|  |  |  |
| --- | --- | --- |
| U.S. Radiocommunications Sector  Fact Sheet | | |
| **Working Party:** ITU-R WP 5B | **Document No:** USWP5B34-xx | |
| **Ref:** 5B/216 Annex 17 | **Date:** February 10, 2025 | |
| **Document Title:** Preliminary Draft New Recommendation ITU-R M.[AMRS-VDL], “Characteristics and protection criteria for the International Civil Aviation Organization standardized VHF datalink Mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136-137 MHz” | | |
| **Author(s)/Contributors(s):**  Chris Tourigny  FAA Spectrum Engineering Services  Sandra Wright  FAA Spectrum Engineering Services  Michael Tran  MITRE | | Phone: 202-267-3071  Email: chris.tourigny@faa.gov  Phone: 202-603-7094  Email: sandra.a.wright@faa.gov  Phone: 703-983-1295  Email : mtran@mitre.org |
| **Purpose/Objective:** The purpose of this contribution is to elevate this Preliminary Draft New Recommendation to Draft New Recommendation. | | |
| **Abstract:** The purpose of this contribution is to elevate this Preliminary Draft New Recommendation to Draft New Recommendation. | | |

|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Source: Document 5B/216 Annex 17  Subject: New Recommendation ITU-R M.[AMRS-VDL] | Document 5B/xxx |
| 29 April 2025 |
| English only |
| United States of America | |
| PRELIMINARY DRAFT NEW RECOMMENDATION ITU-R M. [AMRS-VDL] | |
| Characteristics and protection criteria for the International Civil Aviation Organization standardized VHF datalink Mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136-137 MHz | |

Introduction

This contribution proposes to elevation the Preliminary Draft New Recommendation ITU-R M.[AMRS-VDL], “Characteristics and protection criteria for the International Civil Aviation Organization standardized VHF datalink Mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136-137 MHz” to the Draft New Recommendation.

ATTACHMENT

|  |
| --- |
| ATTACHMENT |
| DRAFT NEW RECOMMENDATION ITU-R M. [AMRS-VDL] |
| Characteristics and protection criteria for the International Civil Aviation Organization standardized VHF datalink Mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136-137 MHz |

(202X)

Scope

This Recommendation provides the technical characteristics and protection criteria for the International Civil Aviation Organization (ICAO) standardized VHF datalink (VDL) Mode 2 (VDL Mode 2) communications systems operating in the aeronautical mobile (route) service (AM(R)S) in the frequency band 136-137 MHz. These technical characteristics and protection criteria should be used for sharing and compatibility studies with VDL Mode 2 systems.

Keywords

AM(R)S, VHF, VDL, protection criteria, air-to-ground communications, ground-to-air communications

Abbreviations/Glossary

AM(R)S: Aeronautical mobile (route) service

ICAO: International Civil Aviation Organization

VDL Mode 2: VHF data link mode 2

VHF: Very high frequency

RR: Radio Regulations

Related ITU Recommendations and Reports

Recommendation

[ITU-R SM.1535](https://www.itu.int/rec/R-REC-SM.1535/en) The protection of safety services from unwanted emissions

The ITU Radiocommunication Assembly,

considering

*a)* that the frequency band 136-137 MHz is currently used by International Civil Aviation Organization (ICAO)-standardized VHF data link Mode 2 (VDL Mode 2) data communications worldwide for air-to-ground, air-to-air, and ground-to-air aeronautical safety communications;

*b)* that aeronautical safety communications are used in all areas that aircraft operate and land, and in all phases of flight;

*c)* that aircraft may be equipped with up to three aeronautical mobile (route) service (AM(R)S) radio stations utilizing a combination of voice and data radios,

recognizing

*a)* that in high aircraft density areas, such as in Europe and North America, the utilization of VHF channels in the 117.975-137 MHz is highly congested;

*b)* that the ICAO develops standards and recommended practices for civil aviation;

*c)* that Annex 10 to the Convention on International Civil Aviation contains standards and recommended practices for aeronautical radiocommunication systems used by civil aviation;

*d)* that the AM(R)S is a safety service;

*e)* that No. **4.10** of Radio Regulations stipulates “Member States recognize that the safety aspects of radionavigation and other safety services require special measures to ensure their freedom from harmful interference; it is necessary therefore to take this factor into account in the assignment and use of frequencies”;

*f)* that Recommendation ITU-R SM.1535 provides a guideline for the protection of safety services from unwanted emissions,

recommends

1 that the technical and operational characteristics of the VDL Mode 2 systems operating in the 136-137 MHz frequency band, allocated to the AM(R)S and described in Annex 1, should be considered for sharing and compatibility studies;

2 that the criterion of interfering signal power to receiver noise power level, *I/N = −6 dB[[1]](#footnote-1)*, should be considered to protect the VDL Mode 2 systems operating in the AM(R)S in the frequency range 136-137 MHz, and that this represents the aggregate protection level if multiple interferers are present.

Annex 1

Technical and operational characteristics of the VHF datalink mode 2 systems operating in the aeronautical mobile (route) service  
in the frequency band 136-137 MHz

# A1.1 Introduction

The frequency band 136-137 MHz is allocated to the AM(R)S and is the principle communications band for aeronautical safety data communications in the air-to-ground, air-to-air, and ground-to-air directions. These systems are internationally standardized by the ICAO for VDL Mode 2. These communications are used in all airspaces where air traffic services are available and in all phases of flight.

# A1.2 Technical characteristics of the VHF datalink mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136‑137 MHz

The technical characteristics of representative VDL Mode 2 systems operating in the frequency band 136-137 MHz are presented in Table A1-1. Some stations use different antennas to transmit and to receive signals.

Table A1-1

Characteristics of VHF data link mode 2 systems operating in the frequency band 136-137 MHz

| Platform | Units | Aircraft | Base station |
| --- | --- | --- | --- |
| Type of emission |  | Data | Data |
| Modulation type |  | D8PSK | D8PSK |
| Type of operation |  | Simplex | Simplex |
| Max antenna height | m | 15 240 (MSL) | 15-50 (AGL) (15 typical) |
| **Transmitter** | | | |
| Power | W | 18 to 25 | Typical 25 |
| Coverage radius | km | 370 | 370 |
| Bandwidth | kHz | 25 | 25 |
| Antenna gain | dBi | 0 | 2.2 |
| Radiation pattern |  | Omni | Omni |
| Antenna polarization |  | Vertical | Vertical |
| Emission mask |  | ICAO SARPs, Annex 10, Vol. III, Part 1, Sections 6.3.3 (RR App. **3**) and 6.3.4 | ICAO SARPs, Annex 10, Vol. III, Part 1, Sections 6.2.3 (RR App. **3**) and 6.2.4 |
| **Receiver** | | | |
| Noise figure | dB | 6 | 6 |
| IF bandwidth | kHz | 25 | 25 |
| Antenna gain | dBi | 0 | 2.2 |
| Radiation pattern |  | Omni | Omni |
| Antenna polarization |  | Vertical | Vertical |

1. This protection criteria does not include safety margin. [↑](#footnote-ref-1)