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	Abstract:   The last WP5C meeting in May 2026 finalized the CPM text for AI 1.10. The US proposed mask made it to the options. The US NGSO mask is equivalent to the one proposed by CEPT. It is methods A3 and A4 of the CPM. CEPT studies showed how the proposed NGSO mask would protect even the worst-case FS elevation, i.e. 10 deg, which is a conservative case for the US. With this input, the US will perform a very similar study as the one performed by CEPT, to reinforce the message that the NGSO mask in methods A3 and A4 is the one to go for, and will conservatively protect FS victims even at 10 deg.
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The last WP5C meeting in May 2026 finalized the CPM text for AI 1.10. The US-proposed NGSO mask is contained method A4 of the CPM text. This mask is equivalent to the one proposed by CEPT and included in method A3. Cept studies submitted to the May 2026 meeting showed how the proposed NGSO mask would protect even the worst-case FS elevation, i.e. 10 deg, which is a conservative case for the US. With this input, the US performed the same study, to reinforce the message that the NGSO mask in methods A3 and A4 will conservatively protect FS victims even at 10 deg, and therefore is the appropriate mask to adopt within AI 1.10.

Study #YZ
This study considers FS characteristics as provided in doc 5C/322 (Annex 2.2) and assuming 10 degrees as maximum elevation. With respect to the parameters of non-GSO systems (including minimum elevation, GSO exclusion zone, and max number of co-frequency beams at a specific location), the analysis considered cases with different operational conditions than those communicated by 4A as described below. The various assumptions different from the 4A liaison statement are on purpose all worse than the parameters communicated by 4A. That said, the assumptions remain within the envelope of parameters agreed as high-level guidance in November 2025 by WP5C. Additionally, the methodology considers scenarios with propagation characteristics as per Doc. 5C/74 (guidance provided by WP 3J and 3M). 
The statistics of the interference power against time for each power flux density (PFD) mask specified is calculated at each timestep using the method described below:
	
1)	Collocate an FSS earth station (ES) with the terrestrial FS station.
2)	Based on the parameters of the selected non-GSO systems, determine number of visible satellites to the FS station,   (satellites above an elevation angle of 0°).
3)	Determine the pool of eligible satellites for each of the selected non-GSO systems complying with the system-specific minimum elevation angle, , and minimum GSO exclusion angle,  at the ES location.
4)	Select maximum number of non-GSO satellites allowed to transmit with overlapping frequencies towards the same location on the ground,  using random satellite selection strategy. Determine the contribution from the  satellites to the FS station.
	             (eq. 1)
		 is the assumed power flux density at the Earth’s surface in dB(W/m2/MHz) under free-space condition
		 is the wavelength in meters
		 is the atmospheric loss (gaseous attenuation) experienced by non-  satellites of NGSO link when performing dynamic simulation. Such propagation loss should be considered based on ITU-R Recommendations ITU-R P.676 when applicable. 
		 is the gain of the FS receiving antenna at off-axis angle  degrees

5)	For the remaining visible   satellites (also known as non- satellites), determine contribution of the sidelobes towards[footnoteRef:1] the FS station assuming random placement of the beams from the satellite with its field of view.  [1:  Sidelobe radiation pattern for each of the visible   satellites of a non-GSO system have been calculated conservatively as per Recommendation ITU-R S.1528 recommends 1.2. In some other working parties’ studies, Recommendation ITU-R S.1528 recommends 1.4 has been considered for sidelobe radiation pattern. The satellite antenna transmit peak gain of  48 dBi, 48 dBi, 51.1 dBi and 52 dBi have been assumed for System B, System D, System L and System M, respectively, with L_n = -20 dB. ] 

 	            (eq. 21)
		 is the assumed effective isotropic radiated density from the non- satellite to the FS station direction in dB(W/MHz) at off-axis angle  degrees. Peak EIRP of the non- satellite is calculated for that satellite to maintain the PFD under free-space condition according to the proposed PFD mask given a randomly selected scan angle within its eligible scan angles.
		is the wavelength in meters
		is the distance between the non- satellite and FS station in meters
		 is the atmospheric loss (gaseous attenuation) experienced by non-  satellites of NGSO link when performing dynamic simulation. 
		 is the gain of the FS receiving antenna at off-axis angle  degrees

6)	Aggregate power levels received at the FS station by combining the received interference power from all  satellites of the non-GSO systems.
7)	Aggregate power levels received at a FS station by combining the received interference power from the selected non-GSO systems. The FS station effective system noise temperature is also increased with atmospheric attenuation according to equation (69) in ITU-R P.618-14 and ITU-R P.676-13 Section 4, when atmospheric effect (gaseous attenuation) is considered in simulation.  

Parameters of the Selected non-GSO Systems
The selected parameters of the selected four non-GSO systems are shown in Table 1. According to the WP4A guidance, 1.5° minimum angular separation is used among the three non-GSO systems’ beams serving the same location on Earth. 
Table 1[footnoteRef:2] [2:  For interference analysis, minimum elevation angle 0° have been considered for the non-GSO systems.] 

Parameters of the Selected GSO and non-GSO Systems (as per 4A guidance)
	GSO/Non-GSO System
	Height
(km)
	Number of planes
	Satellites per plane 
	Inclination angle (deg)
	Number of co-frequency beams, 
	Min. GSO Exclusion angle, 

	System-B (non-GSO)

	590, 610, 630
	28, 36, 34
	28, 36, 34
	33, 42, 51.9
	32
	1°

	System-D (non-GSO)
	1050
	12
	28
	89
	8 (assumed)
	1°

	System-L (non-GSO)
	500, 500, 600, 600, 700, 700, 800, 800, 900, 900, 1000, 1000, 1100, 1100, 1200, 1200, 1300, 1300, 1400, 1400, 8100, 8100, 8100, 8100, 8100, 8100, 8100, 8100, 12000, 12000, 12000, 12000, 12000, 12000, 12000, 12000, 16000, 16000, 16000, 16000, 16000, 16000, 16000, 16000, 20000, 20000, 20000, 20000, 20000, 20000, 20000, 20000, 23222, 23222,
	36, 36, 36, 36, 34, 34, 30, 30, 28, 28, 24, 24, 24, 24, 22, 24, 20, 20, 18, 18, 1, 12, 12, 12, 12, 12, 12, 12, 1, 12, 12, 12, 12, 12, 12, 12, 1, 12, 12, 12, 12, 12, 12, 12, 1, 12, 12, 12, 12, 12, 12, 12, 1, 12
	36, 36, 32, 32, 32, 32, 32, 32, 30, 30, 24, 24, 24, 24, 24, 24, 24, 24, 20, 20, 96, 10, 10, 10, 10, 10, 10, 10, 96, 10, 10, 10, 10, 10, 10, 10, 96, 10, 10, 10, 10, 10, 10, 10, 96, 10, 10, 10, 10, 10, 10, 10, 96, 9
	50, 85, 50, 85, 50, 85, 50, 85, 50, 85, 50, 85, 50, 85, 50, 89, 50, 85, 50, 85, 0, 15, 45, 60, 65, 70, 75, 80, 0, 15, 45, 60, 65, 70, 75, 80, 0, 15, 45, 60, 65, 70, 75, 80, 0, 15, 45, 60, 65, 70, 75, 80, 0, 56
	10
(assumed)
	1°

	System-M (non-GSO)

	340, 345, 350, 360, 525, 530, 535, 604, 614
	12, 18, 48, 48, 48, 30, 28, 28, 28
	110, 110, 110, 120, 120, 120, 120, 12, 18
	53, 46, 38, 97, 53, 43, 33, 148, 116
	40
(assumed)
	1°



This study considers the following operational conditions for the GSO and non-GSO systems: 
· There is a total of 18 identical GSO systems along with the three non-GSO systems. The satellites are assumed to be spaced on the GSO arc every 3° between 22.5°W to 28.5°E. 

·  of System-M is assumed to be 40.

PFD masks
Table 2 lists the pfd mask used in the Study #YZ for the selected non-GSO systems. This is the identical PFD mask proposed by US in 5C/288 as method for the non-GSO FSS to satisfy the agenda item. All satellites that are in view of the FS station are assumed to be possibly interfering satellites for this study. The  satellites transmitting towards the location of FS station are randomly selected from each set of prospective transmitting satellites. 
Table 2 
PFD masks for the Selected non-GSO systems
	PFD in dB(W/m2) for angles of arrival () 
above the horizontal plane
	Reference Bandwidth 


	0°-5°
	5°-12°
	12°-15°
	15°-90°
	

	-125
	-125+1.43()
	-115+3.33()
	-105
	1 MHz


FS Link Characteristics
FS link characteristics has been used following WP 5C guidance as listed in Table 3. 
[bookmark: _Ref126458654]Table 3
FS Link Characteristics
	Parameters
	Specifications

	Frequency (GHz)
	73.5

	FS Antenna maximum Receive Gain (dBi)
	41.5 (0.2 m), 51(0.6 m)

	FS Antenna Pattern
	Rec. ITU-R F.1245-3,
EN 302 217-4 Class-3

	Latitude (degrees)
	24° N, 45° N and 60° N

	Longitude (degrees)
	3° E

	Elevation Angles
	10°

	Receiver Noise Figure (dB)
	8

	Antenna height(m) above mean sea level (AMSL)
	30

	Above mean sea level (AMSL) (m)
	24° N, 3° E: 528 m
45° N, 3° E: 1014 m
60° N, 3° E: 0 m



The protection criteria for FS safeguard used in this analysis are:
[bookmark: _Hlk210124597]a	Long-term:   I/N should not exceed –10 dB for more than 20% of the time (derived from Recommendation ITU-R F.758-8)
b	Short-term:  I/N should not exceed +11 dB for more than 0.00128% of the time in any month.

Results of study # XZ
ITU-R F.1245-3 FS station antenna pattern
Figure 1-6 shows aggregate I/N from the selected four non-GSO systems for
	the ITU-R F.1245-3 FS station antenna pattern, 
	pointing at two different azimuth directions (results can be provided with 20° intervals upon request)
	at a representative frequency (i.e., 73.5 GHz) 	

Figure 1
Aggregate I/N from Selected Systems at 24°N, Azimuth 0°
[image: ]
Figure 2
Aggregate I/N from Selected Systems at 24°N, Azimuth 180°
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Figure  3
Aggregate I/N from Selected Systems at 45°N, Azimuth 0°
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Figure 4
Aggregate I/N from Selected Systems at 45°N, Azimuth 180°
[image: ]


Figure  5
Aggregate I/N from Selected Systems at 60°N, Azimuth 0°
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Figure 6
Aggregate I/N from Selected Systems at 60°N, Azimuth 180°
[image: ]



EN 302 217-4 Class-3FS station antenna pattern
Similarly, Figure 7-12 shows aggregate I/N from the same selected four non-GSO systems for
	the EN 302 217-4 Class-3 FS station antenna pattern, 
	pointing at two different azimuth directions (results can be provided with 20° intervals upon request)
	at same representative frequency (i.e., 73.5 GHz)

 Figure  7
Aggregate I/N from Selected Systems at 24°N, Azimuth 0°
[image: ]
Figure 8
Aggregate I/N from Selected Systems at 24°N, Azimuth 180°
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Figure  9
Aggregate I/N from Selected Systems at 45°N, Azimuth 0°
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Figure 10
Aggregate I/N from Selected Systems at 45°N, Azimuth 180°
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Figure  11
Aggregate I/N from Selected Systems at 60°N, Azimuth 0°
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Figure 12
Aggregate I/N from Selected Systems at 60°N, Azimuth 180°
[image: ]


Conclusion

Dynamic sharing studies using conservative non-GSO parameters (worse than WP 4A guidance), the proposed PFD mask (Table 2), and WP 5C FS characteristics show that aggregate  from the example systems remains within both the long-term ( dB for  of time) and short-term ( dB for  of time) FS protection criteria at all examined latitudes, azimuths, antenna patterns (ITU-R F.1245-3 and EN 302 217-4 Class-3), and gains. The proposed PFD mask therefore protects FS and is suitable for Article 21 under WRC-27 AI 1.10.
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