|  |  |
| --- | --- |
| **US Radiocommunications Sector**  **Fact Sheet** | |
| **Working Party:** WP 5B | **Document No:** USWP5B27-02-FirstDraft |
| **Ref:** Annex 28 to Document 5B/355-E | **Date:** 9 August 2021 |
| **Document Title:** Working document toward a preliminary draft new report ITU-R M.[LED-EMI] “Conditions for the protection of radio receivers installed onboard vessels  against electromagnetic interference from LED lighting systems  and other unintended sources” | |
| **Author(s)/Contributors(s):**  Jerry Ulcek  US Coast Guard, Washington DC  Ross Norsworthy  REC, Inc.  Johnny Schultz  Sev1Tech, Inc. | Phone : (202) 475-3607  E-mail: Jerry.l.Ulcek@uscg.mil  Phone : (727) 515-8025  E-mail: Ross\_Norsworthy@msn.com  Phone : (727) 403-4029  E-mail: johnny.schultz@sev1tech.com |
| **Purpose/Objective:** The purpose of this document is to provide additional information and editorial corrections to the working document toward the preliminary draft new Report ITU-R M.[LED-EMI]. | |
| **Abstract:** This document provides a qualitative and quantitative assessment of the reported problem of LED lighting systems and other sources of unintended interference to radio receivers installed onboard vessels. It also provides technical guidance for the protection of shipborne radiocommunications and radionavigation systems. | |

|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Source: Annex 28 to Document 5B/355-E  Subject: Revision of working document toward preliminary draft new Report ITU-R M.[LED\_EMI] | **USWP5B27-XX** |
| **9 August 2021** |
| **English only** |
| Draft revision of Annex 28 to the Working Party 5B Chairman’s Report | |
| Working document toward a preliminary draft new  Report ITU-R M.[LED-EMI] | |
| Conditions for the protection of radio receivers installed onboard vessels  against electromagnetic interference from light emitting diode lighting systems  and other unintended sources | |

Scope

The purpose of this report is to:

– Identify and describe the problem of electromagnetic interference (EMI) emanating from light emitting diode (LED) lighting systems on marine vessels and the effects of EMI on maritime safety-related systems.

– Quantify the intensity of this problem in technical terms.

– Assess the insufficiency of current EMI standards to address this problem.

– Develop new technical guidance relevant problem and coordinate with relevant standards groups.

– Develop installation guidelines for mariners to minimize degradation from EMI to sensitive radio communications and radio navigation equipment on their vessels.

Keywords

[TBD]

Abbreviations/Glossary

AIS: Automatic identification system

CISPR: Comité International Spécial des Perturbations Radioélectriques

EMI: Electromagnetic interference

GMDSS: Global maritime distress and safety system

GNSS: Global navigation satellite system

GPS: Global positioning system

IEC: International Electrotechnical Commission

LED: Light emitting diode

PER: Packet error rate

RBW: Resolution bandwidth, used in ration measurements

RSSI: Received signal strength indication

Related ITU Recommendations, Reports

Recommendations:

[ITU-R F.699](https://www.itu.int/rec/R-REC-F699/en) Reference radiation patterns for fixed wireless system antennas for use in coordination studies and interference assessment in the frequency range from 100 MHz to 86 GHz

[ITU-R F.1336](https://www.itu.int/rec/R-REC-F.1336/en) Reference radiation patterns of omnidirectional, sectoral and other antennas for the fixed and mobile service for use in sharing studies in the frequency range from 400 MHz to about 70 GHz

[ITU-R M.1371](https://www.itu.int/rec/R-REC-M.1371/en) Technical characteristics for an automatic identification system using time-division multiple access in the VHF maritime mobile band

[ITU-R M.1581](https://www.itu.int/rec/R-REC-M.1581/en) Mathematical models for radiodetermination radar systems antenna patterns for use in interference analyses

[ITU-R M.1903](https://www.itu.int/rec/R-REC-M.1903/en) Characteristics and protection criteria for receiving earth stations in the radionavigation-satellite service (space-to-Earth) and receivers in the aeronautical radionavigation service operating in the band 1 559-1 610 MHz

Reports:

# 1 Introduction

Maritime radiocommunication authorities have received many reports[[1]](#footnote-1) of electromagnetic interference (EMI) emanating from light emitting diode (LED) lighting systems on marine vessels. These reports have been primarily focused on interference to the automatic identification system (AIS) and to VHF marine radios, both of which operate in the 156-162 MHz band and are essential to safety of navigation and safety of life. It was found that most LED lighting systems on marine vessels cause significant desensitization of the receivers of both the AIS and the VHF marine radios, especially when the LED lamps are located in close proximity to the AIS antenna and/or the VHF radio antenna.

# 2 Interference protection criteria for automatic identification system and VHF marine radios from unintended radiation sources

Operational “Minimum sensitivity” requirements for the AIS and for VHF marine radios are developed by ITU and International Electrotechnical Commission (IEC).

For the AIS, the minimum sensitivity is contained in Recommendation ITU-R M.1371 as −107 dBm for a maximum packet error rate (PER) of 20%, which occurs at approximately carrier‑to-interference plus noise ratio = 10 dB (*C*/(*N*+*I*)) = 10 dB, based on the specified co‑channel rejection ratio, which is 10 dB for a PER of 20%. Protection criteria for the VHF data exchange system (VDES), the next generation AIS, are derived in ANNEX 1, which indicates that the VDES protection criteria are approximately 1.3 dB stricter than for the AIS.

For the marine VHF radio, the “maximum useable sensitivity” is contained in IEC 61097-3 edition 2 as “+6 dBµV e.m.f. for a SINAD, psophometrically weighted, of 20 dB”, which occurs at approximately *C*/(*N*+*I*) = 10.8 dB, based on an “FM improvement factor” (FMi) of 9.2 dB, which is determined[[2]](#footnote-2) by:

*FMi* = (*S/N*)o/(*C*/(*N+I*)) = 3(∆*F*/*fm*)2 = 3(5/3)2 = 8.33, logarithmically, 10 log10 8.33 = 9.2 dB

Note that +6 dBµV e.m.f. is equivalent to −107 dBm in a 50-ohm system, since e.m.f. is technically defined as the open-circuit voltage of the energy source. Also note that this level is the same as 2 µV e.m.f. (the open-circuit output terminal of the 50-ohm signal source) and 1 µV at the 50-ohm input terminal of the victim equipment. Therefore, the sensitivity and interference protection criteria for both the AIS and the marine VHF radio are within 0.8 dB:

## 2.1 For the VHF marine radio receiver and the automatic identification system receiver

For the VHF marine radio receiver, the maximum interference plus noise (*I+N*) level, at the input of the receiver is (−107 dBm − 9.2 dB) = −116.2 dBm. Since thermal noise in the VHF marine radio receiver bandwidth of 16 kHz = *N* = kTB = −131.96 dBm, and the maximum level of *I+N* = −116.2 dBm, the maximum level of interference (I) can be calculated from the linear power terms and converted back to logarithmic terms. Consequentially, the maximum level of interference (*I*) at the VHF marine radio receiver input is −116.32 dBm.

And for the AIS receiver, the maximum interference plus noise (*I+N*) level, at the input of the receiver is (−107 dBm – 10 dB) = −117 dBm. Since thermal noise in the AIS receiver bandwidth of 18 kHz = N = kTB = −131.4 dBm, and the maximum level of *I+N* = −117 dBm, the maximum level of interference (I) can be calculated from the linear power terms and converted back to logarithmic terms. Consequentially, the maximum level of interference (I) at the AIS receiver input is −117.16 dBm. Thus, protection for the AIS will ensure protection for the VHF marine radio receiver.

### 2.1.1 Assessing the efficacy of the current electromagnetic interference standards for this application

The current EMI standards specify a maximum field strength level measured at a separation distance.

Example 1: IEC 60945 specification (per 9 kHz bandwidth):

– Maximum field strength level (quasi-peak): 24 dBµV/m = 16 µV/m

– Separation distance for measurement: 3 meters

Example 2: CISPR 25 Class 5 specification (per 120 kHz bandwidth):

– Maximum field strength level (average): 15 dBµV/m = 5.6 µV/m

– Maximum field strength level (quasi-peak): 22 dBµV/m = 12.6 µV/m

– Separation distance for measurement: 1 meter

Note that the Comité International Spécial des Perturbations Radioélectriques (CISPR) measurement bandwidths for the VHF marine frequency band (156-162 MHz) is 120 kHz and the IEC 60945 measurement resolution bandwidth (RBW) for this band is 9 kHz. Considering that the VHF marine radio receiver bandwidth is 16 kHz, and the AIS receiver bandwidth is 18 kHz, testing in a 20 kHz resolution bandwidth will more accurately assess the performance effects on both of these maritime VHF receivers. For example, it was found that changing from 120 kHz bandwidth to the IEC 60945 specified 9 kHz bandwidth, “the test level of the marine VHF band will decrease 16-20 dB for most signals” [[3]](#footnote-3). This measurement bandwidth factor is considered in Section 3.1.3.1 below.

### 2.1.2 Information needed for this application

– Separation distances between victim antennas and unintentional interference sources, e.g., for LED navigation lights:

NOTE: The separation distance, for this analysis, is the distance between the interfering device and the center of radiation of the victim antenna. The antenna gain for this analysis may also be adjusted (see graph in Figure 1) to account for the angular offset to the antenna radiation pattern relative to the reference elevation angle of zero degrees (00).

Worst case = 1 meter; edge of antenna near-field, minimum separation. In rare cases = 0.5 meter; in the antenna near-field, should be avoided if possible. Characteristics of the victim equipment antennas are shown in Figure 1 below:

Figure 1

Characteristics for vertical whip antennas based on Recommendation ITU-R F.1336[[4]](#footnote-4)

NOTE: Antenna gain is defined as the gain at 00 elevation angle.

– For the AIS, the typical antenna is a 4-foot whip; gain= +2 dBi = 0 dBd.

– For the VHF radio, the typical antenna is an 8-foot whip; gain = +6 dBi = 3 dBd.

### 2.1.3 Necessary adjustments to current standards to fit this application

Adjustments to field strength level

– Adjustment for distance separation: 20log10 D, in meters

– Adjustment for marine VHF radio is based on receiver sensitivity and antenna characteristics (gain, radiation pattern and angular offset of the position of the interfering source relative to the antenna)

– Adjustment for AIS is based on receiver sensitivity and antenna characteristics (gain, radiation pattern and angular offset of the position of the interfering source relative to the antenna)

– Consideration of the measurement resolution bandwidth compared to the bandwidth of the victim receiver, based upon the type of detector used to measure interference (e.g., average, quasi-peak and peak) and the type of interference encountered, as noted in Section 2.1.3.2 and 2.1.3.5.

– Adjustment for reactive near field effect in partially illuminating a 2.5 m shipboard VHF marine radio antenna, for example, from an unintentional emitter separated by as little as 1 m or even 0.3 meters, as noted in ANNEX 2. The reactive near field for such an antenna begins at 1.5 m separation.

#### 2.1.3.1 Field strength determination examples for the automatic identification system

Maximum interference signal level at the AIS RF input terminal = −117.16 dBm

The conversion of maximum interference power level to maximum interference field strength level is as follows:

NOTE: Units are assumed to be rms values (average values, not quasi-peak values).

Method 1 (standard method)

E dBµV/m = AF dB/m + V dBµV

AF50Ω = 20 log10 fMHz – 10 log10 G – 29.7707, where

G = 1.64 for the 0 dBd AIS antenna

AF50Ω = 44.19 – 2.15 – 29.7707 = 12.27 dB/m

V dBµV (for -117.16 dBm) = -10.17 dBµV

E dBµV/m = AF dB/m + V dBµV = 12.27 – 10.17 = +2.1 dBµV/m

Method 2 (according to: Wikipedia, Antenna Factor)

AF50Ω = 9.73/(λ√G) = 4.10/m = 12.26 dB/m

and

AF = E/V

Thus

AFdB/m = EdBV/m – VdBV = EdBµV/m - VdBµV

EdBµV/m = AFdB/m + VdBµV = 12.26 + (-10.17) = +2.1 dBµV/m

**Result:** The results of Method 1 and Method 2 are identical.

#### 2.1.3.2 Adjustments for standard resolution bandwidth

Ideally, if the spectral distributions of all interference sources could be assumed to be Gaussian, a test standard with an RBW of B1 could be adjusted to a victim receiver with effective receiver bandwidth B2, by adjusting the test levels according to L1/L2 = 10 log (B1/B2) as shown below. Units are assumed to be average values (not peak or quasi-peak values). However, it has been found that this test bandwidth adjustment does not accurately represent the interference scenario in the VHF maritime environment, as previously noted in Section 2.1.1, and as further evidenced by the test results reported in Section 2.1.3.5.

**Adjustments based on Gaussian interference spectrum:**

**For a 9 kHz resolution bandwidth, per IEC 60945**

PdBm = -117.16 + 10 log (9/18) = -120.16 dBm

P dBm   = V dB uV – 107

V dBµV (for -120.16 dBm) = -120.16 + 107 = -13.16 dBµV

E dBµV/m = 12.27 + (-13.16) = **-0.89 dBµV/m**

**For a 20 kHz resolution bandwidth, for VHF maritime 25 kHz channels[[5]](#footnote-5)**

PdBm = -117.16 + 10 log (20/18) = -116.70 dBm

P dBm   = V dB uV – 107

V dBµV (for -116.70 dBm) = -116.70 + 107 = -9.70 dBµV

E dBµV/m = 12.27 + (-9.70) = **+2.57 dBµV/m**

**For a 120 kHz resolution bandwidth, per CISPR 25 Class 5**

PdBm = -117.16 + 10 log (120/18) = -108.92 dBm

P dBm   = V dB uV – 107

V dBµV (for -108.92 dBm) = -108.92 + 107 = -1.92 dBµV

E dBµV/m = 12.27 + (-1.92) = **+10.35 dBµV/m**

#### 2.1.3.3 Comparing these levels to current standards

– CISPR 25 Class 5 (120 kHz bandwidth and 1 meter):

• Maximum field strength level (average): +15 dBµV/m

The minor difference (15 dBµV/m -10.35 dBµV/m = 4.65 dB) between the CISPR 25 Class 5 level and the level calculated for the AIS may be attributed to the higher gain (physical size) of the typical marine antenna compared to the typical automotive antenna addressed by CISPR 25 Class 5.

• Maximum field strength level (quasi-peak): +22 dBµV/m

• Maximum field strength level (peak): +35 dBµ

– IEC 60945 (9 kHz bandwidth and 3 meters):

• Maximum field strength level (quasi-peak): +24 dBµV/m

#### 2.1.3.4 Measurements in a typical electromagnetic interference laboratory test chamber

For the 9 kHz resolution bandwidth, the ambient noise floor (kTB) is:

PdBm (kTB for 9 kHz resolution bandwidth) = -134.43 dBm

For the test chamber:

The noise figure of the measurement system is 3.0 dB.

The antenna factor of the test antenna is 14.7 dB/m.

Therefore:

P dBm = (kTB + NF) = -134.43 + 3 = -131.43 dBm

V dBµV (for -131.43 dBm) = -131.43 + 107 = -24.43 dBµV

E dBµV/m = 14.7 + (-24.43 dBµV) = -9.73 dBµV/m

Thus, the ambient level of the chamber, -9.73 dBµV/m, is 8.84 dB below the test level, -0.89 dBµV/m, which meets the 6 dB CISPR minimum requirement.

Test results from the test chamber (ambient level, average level measurement) shown in Figure 2 below are consistent with the calculated value (-9.73 dBµV/m) shown above. Thus, it is practical to measure the levels required to protect the AIS in a typical EMI test laboratory, e.g. footnote 6.

Figure 2

Measurement of the ambient noise level (9 kHz resolution bandwidth, fast fourier transform, average level) of the electromagnetic interference test chamber[[6]](#footnote-6)

Text, application

Description automatically generated

#### 2.1.3.5 Results from testing numerous maritime LEDs in the electromagnetic interference laboratory test chamber

Figure 3 provides a summary of test results from testing radiation from numerous samples of marine LED lights in the EMI laboratory test chamber referred to in footnote 6. The samples were tested in the resolution bandwidths of 9 kHz, 20 kHz, and 120 kHz noted in Section 2.1.3.2 above, using average, peak, and quasi-peak detectors. Only the results from the “active”[[7]](#footnote-7) samples is recorded here because the others did not radiate above the ambient noise level of Figure 2.

Figure 4 provides a comparison of measured radiation levels as a function of resolution bandwidth.

ANNEX 2 provides measured effects of radiation from the “active” sample LED lights on the installed victim receivers, VHF marine radio, and AIS, at various installed separation distances from 0.33 meters to 3 meters.

**Conclusions:**

The conclusions from these test results represented in Figure 3, Figure 4, and ANNEX 2 are:

* Only Sample 1 passes CISPR 25 Class 5 level of +15 dBµV/m average in 120 kHz RBW.
* None of the samples pass any of the levels stated in Section 2.1.3.2 above, but sample 1 comes the closest, within 5 dB.
* The relationship between measured levels and RBW is inconsistent, thus unpredictable.
* Although it is difficult to come to a precise conclusion, the tests performed in ANNEX 2 support the adequacy of the predicted radiated emission limit of +2.57 dB µV/m average at 20 kHz RBW and one meter separation, calculated in Section 2.1.3.2, to protect the VHF radio and AIS.

Figure 3

**Test results from “active” samples**

Chart, bar chart

Description automatically generated

FIGURE 4

**Comparison of measured radiation levels as a function of resolution bandwidth**

# Chart, bar chart Description automatically generated3 Interference protection criteria for marine global navigation satellite system receivers from unintended radiation sources

The interference protection criteria for global navigation satellite system (GNSS) (e.g., global positioning system (GPS)) receivers may be based on Recommendation ITU-R M.1903 *Characteristics and protection criteria for receiving earth stations in the radionavigation-satellite service (space-to-Earth) and receivers in the aeronautical radionavigation service operating in the band 1 559-1 610 MHz*

Acquisition mode threshold power density level of aggregate wideband interference at the passive antenna output:      **−142 dB W/MHz = -112 dBm/MHz**

Tracking mode threshold power density level of aggregate wideband interference at the passive antenna output:      **−136 dB W/MHz = -106 dBm/MHz**

Acquisition mode threshold power level of aggregate narrow-band interference at the passive antenna output: **−158 dBW = 128 dBm**

*[Editor’s note: Antenna gain is not applied in this analysis because it equally affects both signal and interference.]*

RF filter 3 dB bandwidth: **32 MHz**

Pre-correlation filter 3 dB bandwidth: **2 MHz**

Noise temperature: **645oK**

AF50Ω = 20 log10 fMHz – 10 log10 Gnumeric – 29.7707 dB/m,

                              = 63.945 – 29.7707 = 34.174 dB/m at 1 575 MHz

P dBm   = V dB uV – 107

E dB µV/m = AF50Ω + V dB µV= AF50Ω + P dBm + 107 = P dBm + 107 + 34.174 = P dBm + 141.174

## 3.1 Adjustments for standard resolution bandwidth

For a 1 MHz resolution bandwidth

P dBm (acquisition) = -112 dBm/MHz

E dB µV/m (acquisition) = -112 dBm + 141.174 = 29.2 dBµV/m

For a 120 kHz resolution bandwidth

P dBm (acquisition) = -112 dBm – 10 log (1/0.120) = -112 -9.2 = -121.2 dBm

E dB µV/m (120 kHz) = -121.2 dBm + 141.174 = 20 dBµV/m

For a 9 kHz resolution bandwidth

P dBm (acquisition) = -112 dBm – 10 log (1/0.009) = -112 -20.46 = -132.46 dBm

E dB µV/m (9 kHz) = -132.46 dBm + 141.174 = 8.71 dBµV/m

**3.2 EMC protection criteria based upon Rec. ITU-R M.1903 narrowband interference**

E dB µV/m = AF50Ω + V dB µV= AF50Ω + P dBm + 107 (field strength 1m from the   
antenna)  
E dB µV/m = P dBm + 107 + 34.175 = P dBm + 141.175 (GPS and Galileo)

E dB µV/m = P dBm + 107 + 34.322 = P dBm + 141.323 (GLONASS)

P dBm (NBacquisition) = -128 dBm (GPS and Galileo)  
P dBm (NBacquisition) = -128 dBm (GLONASS)

E dB µV/m (NBacquisition) = -128 dBm + 141.175 = 13.2 dB µV/m (GPS and Galileo)

E dB µV/m (NBacquisition) = -128 dBm + 141.323 = 13.3 dB µV/m (GLONASS)

## 3.3 Comparing these levels to current standards[[8]](#footnote-8)

– IEC 60945 (120 kHz, quazi-peak, 3 meters): 54 dB µV/m

• Adjustment for 3 meters to 1 meter: 20 log (3/1) = + 9.54 dB

• Adjustment for quazi-peak to average: - 10 dB[[9]](#footnote-9)

• Adjusted value: + 54 - 10 + 9.54 = 53.5 dBµV/m

• Difference to this calculation: 53.5 – 20 = 33.5 dB

– CISPR 25 Class 5 (9 kHz, 1 meter, average): 10 dBµV/m

• Difference to this calculation: 10 – 8.71 = 1.29 dB

### 3.3.1 Results of comparison to current standards

Recommendation ITU-R M.1903 requires the acquisition mode threshold power density level of aggregate wideband interference at the passive antenna output to be no greater than -142 dB W/MHz. This level is only 1.83 dB above kTB (kTB = -143.83 dB W/MHz), which can only be measured with specialized equipment including very high gain antenna and very low noise preamplifier, as noted below.

### 3.3.2 Measurements by an electromagnetic interference certification laboratory

**For a typical EMI laboratory test chamber:**

For the 9 kHz RBW, the ambient noise floor (kTB) is:

PdBm (kTB for 9 kHz resolution bandwidth) = -134.43 dBm

The noise figure of the typical measurement system is 3.0 dB.

The antenna factor of the typical test antenna is 25.0 dB/m.

Therefore:

P dBm = (kTB + NF) = -134.43 + 3 = -131.43 dBm

V dBµV (for -131.43 dBm) = -131.43 + 107 = -24.43 dBµV

E dBµV/m = 25.0 + (-24.43 dBµV) = +0.57 dBµV/m

Thus, the ambient level of the chamber, +0.57 dBµV/m, is only 8.14 dB below the test level, +8.71 dBµV/m, which barely meets the 6 dB CISPR minimum requirement, but it does not allow for measurement uncertainty of typically 3 dB.

**Enhancements for testing to Recommendation ITU-R M.1903**

Example enhancements for the EMI laboratory test chamber:

The noise figure of the special low noise preamplifier[[10]](#footnote-10) at 1575 MHz is 1.5 dB.

The antenna factor of the special high gain horn test antenna[[11]](#footnote-11) at 1575 MHz is:

AF50Ω = 20 log10 fMHz – GdB – 29.7707 dB/m; GdB = 14.4dB; AF50Ω = 19.77dB/m

Therefore:

P dBm = (kTB + NF) = -134.43 + 1.5 = -132.93 dBm

V dBµV (for -132.93 dBm) = -132.93 + 107 = -25.93 dBµV

E dBµV/m = 19.77 + (-25.93 dBµV) = -6.16 dBµV/m

The ambient level of the enhanced EMI laboratory test chamber, -6.16 dBµV/m, is 14.87 dB below the test level, +8.71 dBµV/m. This meets the 6 dB CISPR minimum requirement with a comfortable margin, including measurement uncertainty of typically 3 dB.

### 3.3.3 Conclusion

Testing to the level prescribed by Recommendation ITU-R M.1903 by a certified EMI test laboratory may require some enhancements as noted in the example stated above.

# 4 Summary of Results

If these lighting systems are installed on marine vessels, installers should use the following guidelines to avoid unintended interference to safety related marine radio communications (both HF and VHF) and radio-navigation systems (both AIS and GPS).

## 4.1 Important Precautions for avoiding interference when using light emitting diode lamps

If LED lamps are used, ensure they are proven to meet CISPR 25 Class 5 radiated emissions limits in the marine radio communications and radio-navigation frequency bands, measured at 1 meter from the LED lamps:

– HF Marine Band (RR Appendix **17**) 2-30 MHz: 20 dB(µV/m) average

– VHF Marine Band (RR Appendix **18**) 156-162 MHz: 15 dB(µV/m) average

– GNSS L1 Marine Band (1 559-1 610 MHz): 10 dB(µV/m) average

## 4.2 Separate light emitting diode lamps from sensitive antennas

To mitigate EMI from LED lamps, separate the LED lamps as far as possible from VHF marine band antennas, with a minimum distance of 1 meter wherever possible.

## 4.3 Use vertical separation wherever possible

If possible, separate the LED lamps from the sensitive antennas in the vertical direction, either over or under each other, in order to minimize the coupling between them. Refer to the antenna patterns on Figure 1 for +/- 90 degrees elevation angle.

## 4.4 Testing for interference following installation[[12]](#footnote-12)

Test the VHF marine radio for interference

To simply test for the presence of EMI, switch off all lighting that could be a source of EMI. Tune the radio to a weak continually broadcasting station. Turn on the LED light(s) one at a time, and then all on. If the broadcast signal vanishes after a lamp is energized, it is generating RF interference.

Alternative method using received signal strength indication to test the VHF marine radio for interference

Marine radios typically use received signal strength indication (RSSI) displays to indicate the strength of a received signal on the radiocommunications channel. The RSSI level is usually displayed in a bar graph.

When a marine radio is tuned to a communications channel that displays an RSSI level but has no discernible output signal, the RSSI level may be an indication of RF interference. To confirm this, the user may lower the squelch control to its minimum setting to determine whether the displayed RSSI level is due to a weak communication signal. This test should be performed on a channel in which there is currently no radio traffic, i.e., a channel that is “quiet” at the time of the test. This condition may occur at night when navigation lights are switched ON. LED lights are a common source of radio interference, and if they are the suspected source of interference, they should be momentarily be switched OFF to determine whether the interference ceases.

Test the automatic identification system for interference

If the AIS antenna is closer to an LED lamp than the VHF marine radio antenna, disconnect the AIS antenna from the AIS and connect it to the marine VHF radio and rerun the test in 4.4 above to verify that the AIS antenna is not degraded. If that is impractical, performing these tests using a VHF handheld in the vicinity of an AIS antenna is a reasonable substitute.

Test the global navigation satellite system for interference

Turn off the LED lamps and note the indicated GNSS S/N values on the various satellites. Turn on the LED lamps, wait ten minutes and then observe whether the GNSS S/N values on the satellites have degraded significantly.

**ANNEX 1**

**Protection criteria for the VHF Data Exchange System (VDES)[[13]](#footnote-13)**

1. **VDES satellite system characteristics**

Protection criteria for the VDES satellite system characteristics described in Rec. ITU-R M.2092 as follows.  The maximum satellite e.i.r.p as a function of elevation angle PFD on ground at 0º elevation (S) is -149 dBW/m2/4 kHz. Note that this is a maximum value and that the actual value based on the VDES satellite’s antenna pattern (8 dB circularly polarized Yagi antenna) is 3.4 dB lower as shown in Table 1 below. Thus, the protection criteria should be based on -152.4 dBW/m2/4 kHz. 

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Ship elevation angle (degrees)** | **Satellite antenna gain**  **(dBi)** | **Nadir offset angle (deg)** | **Boresight offset angle (deg)** | **Satellite e.i.r.p. in circular polarization (dBW per 50 kHz)** | **Margin to maximum satellite e.i.r.p,**  **i.e margin to the pfd-mask**  **(dB)** |
| 0 | 8 | 66.1 | 0 | −1.4 | 3.4 |
| 10 | 8 | 64.2 | 1.9 | −1.4 | 1.7 |
| 20 | 8 | 59.2 | 6.9 | −1.4 | 0.4 |
| 30 | 7.8 | 52.3 | 13.8 | −1.6 | 0.0 |
| 40 | 6.9 | 44.4 | 21.7 | −2.5 | 0.8 |
| 50 | 5.5 | 36 | 30.1 | −3.9 | 4.1 |
| 60 | 3.6 | 27.2 | 38.9 | −5.8 | 10.5 |
| 70 | 0.7 | 18.2 | 47.9 | −8.7 | 13.7 |
| 80 | −2.2 | 9.1 | 57 | −11.6 | 17.2 |
| 90 | −5.5 | 0 | 66.1 | −14.9 | 21.4 |

Table 1 – Satellite e.i.r.p. and margin to the pfd-mask as a function of elevation angle

1. **VDES satellite downlink budget**

The nominal signal level C/N0 and C/(N0+I0) for the VDE-SAT downlink as a function of elevation angle for a 50 kHz channel are provided in Table 2. In a 50 kHz channel a signal bandwidth of 42 kHz can be used, which allow a satellite transmitter RF output power of -10.2 dBW. A transmission frequency of 161.9125 MHz is used in the calculation of path loss. The ship antenna gain is 3 dBi at zero degrees elevation angle and the system noise temperature is 30.2 dBK. The noise density level (N0) will then be -168.4 dBm/Hz. The link budget shown in Table 2 assumes a maximum noise plus interference density level (N0+I0) of -161 dBm/Hz, based on IEC 61993-2 performance requirements for maritime VHF equipment. Propagation effects, e.g., multi-path fading, are addressed in Section 3.1 of Report ITU-R M.2435-0.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Ship elevation angle**  **(degrees)** | **Satellite EIRP in circular polarization**  **(dBW)** | **Satellite range**  **(km)** | **Path loss**  **(dB)** | **Polarization loss**  **(dB)** | **Ship antenna gain**  **(dBi)** | **Carrier level at LNA**  **(dBm in 50 kHz)** | ***C*/*N0***  **(dBHz)** | ***C*/(*N0*+*I0*) (dBHz)** |
| 0 | −2.2 | 2 829 | 145.7 | 3 | 3 | -117.8 | 50.5 | 43.2 |
| 10 | −2.2 | 1 932 | 142.4 | 3 | 3 | -114.5 | 53.8 | 46.5 |
| 20 | −2.2 | 1 392 | 139.5 | 3 | 2.5 | -112.2 | 56.2 | 48.8 |
| 30 | −2.4 | 1 075 | 137.3 | 3 | 1 | -111.6 | 56.7 | 49.4 |
| 40 | −3.3 | 882 | 135.5 | 3 | 0 | -111.8 | 56.5 | 49.2 |
| 50 | −4.7 | 761 | 134.3 | 3 | −1.5 | -113.4 | 54.9 | 47.6 |
| 60 | −6.6 | 683 | 133.3 | 3 | −3 | -115.9 | 52.5 | 45.1 |
| 70 | −9.5 | 635 | 132.7 | 3 | −4 | -119.1 | 49.2 | 41.8 |
| 80 | −12.4 | 608 | 132.3 | 3 | −10 | -127.7 | 40.7 | 33.3 |
| 90 | −15.7 | 600 | 132.2 | 3 | −20 | -140.9 | 27.5 | 20.1 |

Table 2 – VHF data exchange satellite downlink budget as a function of elevation angle

1. **VDES satellite downlink power flux density and noise plus interference levels**

Satellite PFD and signal power density levels on ground in standard EMI test bandwidths:

PdBm/m2/kHz = -152.4 dBW/m2/4 kHz = -122.4 dBm/m2/4kHz – 10 log 4 = -128.4 dBm/m2/kHz  
PdBm/m2 (9 kHz)   = -128.4 dBm/m2/kHz + 10 log 9    = -128.4 + 9.5   =  -118.9 dBm/m2

PdBm/m2 (20 kHz)  = -128.4 dBm/m2/kHz + 10 log 20  = -128.4 + 13    =  -115.4 dBm/m2

PdBm/m2 (120 kHz) = -128.4 dBm/m2/kHz +10 log 120 = -128.4 + 20.8  =  -107.6 dBm/m2

Antenna effective area Ae for ½ wave dipole = 0.1305λ2 = 0.448 m2 = -3.5 dB (m2){\displaystyle \lambda }

Carrier level CdBm = PdBm/m2 + Ae dB (m2)

CdBm (9 kHz)   = -118.9 dBm/m2 – 3.5 dBm (m2) = -122.4 dBm

CdBm (20 kHz)  = -115.4 dBm/m2 – 3.5 dBm (m2) = -118.9 dBm

CdBm (120 kHz) = -107.6 dBm/m2 – 3.5 dBm (m2) = -111.1 dBm

Maximum noise plus interference density (N0+I0) levels based on (N0+I0) = -161 dBm/Hz:

N0+I0 dBm (9 kHz)   = -161 dBm/Hz + 10 log 9 kHz = -161 + 39.5 = -121.5 dBm

N0+I0 dBm (20 kHz)  = -161 dBm/Hz + 10 log 20 kHz = -161 + 43 = -118 dBm

N0+I0 dBm (120 kHz) = -161 dBm/Hz + 10 log 120 kHz = -161 + 50.8 = -110.2 dBm

Carrier to noise plus interference C/(N0+I0)levels in standard EMI test bandwidths:

C/(N0+I0)(9 kHz)   = -122.4 – (-121.5) = -0.9 dB

C/(N0+I0) (20 kHz)  = -118.9 – (-118) = -0.9 dB

C/(N0+I0) (120 kHz) = -111.1 – (-110.2) = -0.9 dB

Note that the VDES satellite downlink waveform is designed to operate with the prescribed PDF mask in a controlled interference environment.

The conversion of maximum interference power level to maximum interference field strength level can be determined from the following formulae:

NOTE: Units are assumed to be rms values (average values, not quasi-peak values).

Field strength E dBµV/m = AF dB/m + V dBµV

Antenna factor AF50Ω = 20 log10 fMHz – 10 log10 G – 29.7707, where

Antenna gain G = 1.64 (for the 0 dBd AIS antenna)

Therefore AF50Ω = 44.19 – 2.15 – 29.7707 = 12.27 dB/m

And thus E dBµV/m = AF dB/m + V dBµV

1. **Protection criteria for the VDES satellite downlink (refer to ITU-R M.2092)**

For standard EMI test bandwidths 9 kHz and 120 kHz, 20 kHz is added for comparison to the AIS protection criteria:

**For a 9 kHz RBW, per IEC 60945**

PdBm = -121.5 dBm

P dBm   = V dB uV – 107

V dBµV (for -121.5 dBm) = -121.5 + 107 = -14.5 dBµV

E dBµV/m = 12.27 + (-14.5) = **-2.23 dBµV/m**

**For a 20 kHz RBW, for VHF maritime 25 kHz channels (RR Appendix 18)**

PdBm = -118 dBm

P dBm   = V dB uV – 107

V dBµV (for -118 dBm) = -118 + 107 = -11 dBµV

E dBµV/m = 12.27 + (-11) = **+1.27 dBµV/m**

**For a 120 kHz RBW, per CISPR 25 Class 5**

PdBm = -110.2 dBm

P dBm   = V dB uV – 107

V dBµV (for -110.2 dBm) = -110.2 + 107 = -3.2 dBµV

E dBµV/m = 12.27 + (-3.2) = **+9.07 dBµV/m**

1. **Protection criteria for the AIS (refer to Section 2.1.3.2):**

Standard resolution bandwidths for EMI testing are 9 kHz and 120 kHz. The 20 kHz resolution bandwidth and the associated level used for the AIS are based on the AIS test standard, IEC 61993-2, since AIS is a 25 kHz channelized maritime VHF safety system. The levels for the 9 kHz and the 120 kHz resolution bandwidths, are calculated from the 20 kHz level, assuming a Gaussian power flux density for the interference, which typically is not the case since the highest levels of interference on ships are typically from switch-mode power supplies with various non-Gaussian waveforms.

**For a 9 kHz RBW, per IEC 60945**

PdBm = -120.16 dBm

P dBm   = V dB uV – 107

V dBµV (for -120.16 dBm) = -120.16 + 107 = -13.16 dBµV

E dBµV/m = 12.27 + (-13.16) = **-0.89 dBµV/m** *(see footnote 1)*

**For a 20 kHz RBW, for VHF maritime 25 kHz channels (RR Appendix 18)**

PdBm = -116.70 dBm

P dBm   = V dB uV – 107

V dBµV (for -116.70 dBm) = -116.70 + 107 = -9.70 dBµV

E dBµV/m = 12.27 + (-9.70) = **+2.57 dBµV/m**

**For a 120 kHz RBW, per CISPR 25 Class 5**

PdBm = -108.92 dBm

P dBm   = V dB uV – 107

V dBµV (for -108.92 dBm) = -108.92 + 107 = -1.92 dBµV

E dBµV/m = 12.27 + (-1.92) = **+10.35 dBµV/m** *(see footnote 1)*

1. **Conclusions:**

In summary, as shown below, the protection criteria for the VDES Satellite downlink are nearly the same, approximately 1.3 dB stricter than for the AIS.

For protection of the AIS:

For a 9 kHz bandwidth: E dBµV/m = 12.27 + (-13.16) = **-0.89 dBµV/m** [[14]](#footnote-14)

For a 20 kHz bandwidth: E dBµV/m = 12.27 + (-9.70) = **+2.57 dBµV/m**

For a 120 kHz bandwidth: E dBµV/m = 12.27 + (-1.92) = **+10.35 dBµV/m [[15]](#footnote-15)**

For protection of the VDES satellite downlink:

For a 9 kHz bandwidth: E dBµV/m = 12.27 + (-14.5) = **-2.23 dBµV/m**

For a 20 kHz bandwidth: E dBµV/m = 12.27 + (-11) = **+1.27 dBµV/m**

For a 120 kHz bandwidth: E dBµV/m = 12.27 + (-3.2) = **+9.07 dBµV/m [[16]](#footnote-16)**

**ANNEX 2**

**VHF and AIS Installation[[17]](#footnote-17) EMC Test Results**

VHF and AIS installation tests were undertaken with two purposes:

1. To measure the radio systems’ required interference protection criteria, what level of interfering field strength degrades the performance of installed VHF radio and AIS systems. This measurement could be used to validate predicted protection criteria with measured results, and
2. to measure the affect placement of an interfering source has at various distances from a victim antenna, within its near field.

To accomplish this, the radiated emission from 9 light test samples were measured at 1m distance at the operating frequency of both the VHF radio (156.75 MHz) and AIS (161.975 and 161.025 MHz), using an average detector and a resolution bandwidth of both 20 kHz and 120 kHz. The receiver sensitivity of a VHF radio using a 4’ and then an 8’ whip, and an AIS using a 4’ whip, installed in the test chamber was then measured. Receiver sensitivity was measured in accordance with the relevant IEC receiver test standard, with each of the light test samples activated, at distances of 3m, 2m, 1m, 0.66m and 0.33m from the receiver whip antenna.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Light Sample Number** | **No LED** | | **3 meter antenna set back** | | **2 meter antenna setback** | | **1 meter antenna setback** | | **0.66 meter antenna setback** | | **0.33 meter antenna setback** | |
| **Power in dBm** | | | | | | | | | | | |
| **4' WHIP** | **8' WHIP** | **4- WHIP** | **8' WHIP** | **4- WHIP** | **8' WHIP** | **4- WHIP** | **8' WHIP** | **4- WHIP** | **8' WHIP** | **4' WHIP** | **8' WHIP** |
| 1 | -116.5 | -116.5 | -114.5 | -116.5 | -115.5 | -116.5 | -116.5 | -116.5 | -116.5 | -116.5 | -115.5 | -116.5 |
| 2 | -116.5 | -116.5 | -114.5 | -115.5 | -114.5 | -114.5 | -112.5 | -114.5 | -111.5 | -113.5 | -108.5 | -113.5 |
| 3 | -116.5 | -116.5 | -110 | -114.5 | -109.5 | -113.5 | -106.5 | -111.5 | -105.5 | -110.5 | -104.5 | -110.5 |
| 4 | -116.5 | -116.5 | -109.5 | -112.5 | -113.5 | -115.5 | -113.5 | -113.5 | -109.5 | -114.5 | -105.5 | -114.5 |
| 5 | -116.5 | -116.5 | -80 | -91.0 | -84 | -78.0 | -73 | -77.0 | -71 | -82.0 | -68 | -86.0 |
| 6 | -116.5 | -116.5 | -107.5 | -111.5 | -110.5 | -115.5 | -109.5 | -115.5 | -104.5 | -114.5 | -100.5 | -114.5 |
| 7 | -116.5 | -116.5 | -107 | -108.0 | -108 | -109.0 | -108 | -109.0 | -106 | -108.0 | -106 | -108.0 |
| 8 | -116.5 | -116.5 | -114.5 | -114.5 | -114.5 | -115.5 | -113.5 | -115.5 | -113.5 | -112.5 | -112.5 | -112.5 |
| 9 | -116.5 | -116.5 |  | -115.5 |  | -116.0 |  | -116.0 |  | -116.0 |  | -116.0 |
| 10 | -116.5 | -116.5 | -109.5 | -106.5 | -110.5 | -115.5 | -112.5 | -106.5 | -105.5 | -103.5 | -97.5 | -102.5 |

Table 1 - VHF Radio Installation SINAD Test

It is immediately apparent from Table 1 that interference increases as a noisy LED is placed closer to a 4 foot (1.5m) whip antenna, even as close as a foot (0.33m) from the antenna. In light sample #5 for example, interference from that light increases by 2 dB when the light is moved from a meter to 0.66m from the antenna, and then increases another 3 dB when moved from 0.66m to 0.33m from the antenna. The same is not true for an 8 foot (2.5m) antenna. Maximum susceptibility appears to occur 1m from the antenna. Interference from light sample #5 actually decreases by 5 dB when the light is moved within 0.66m of the antenna, and decreases further by another 4 dB when moved to within 0.33m of the antenna.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Light Sample Number | AIS Radio Test ( 4' WHIP ANTENNA) Power in dBm | | | | | |
| No LED | 3 meter Antenna set back | 2 meter Antenna setback | 1 meter Antenna setback | 0.66 meter Antenna setback | 0.33 meter Antenna setback |
| 1 | -112 | -108 | -110 | -110 | -109 | -109 |
| 2 | -112 | -109 | -109 | -107 | -108 | -107 |
| 3 | -112 | -110 | -111 | -110 | -108 | -108 |
| 4 | -112 | -111 | -112 | -110 | -109 | -109 |
| 5 | -112 | -95 | -94 | -89 | -89 | -91 |
| 6 | -112 | -108 | -110 | -111 | -111 | -107 |
| 7 | -112 | -108 | -109 | -109 | -108 | -108 |
| 8 | -112 | -111 | -110 | -110 | -110 | -110 |
| 9 | -112 | -109 | -109 | -112 | -112 | -110 |
| 10 | -112 | -110 | -110 | -107 | -106 | -102 |

Table 2 - AIS Radio Installation Test

The VHF radio and AIS loss of receiver sensitivity shown in Tables 1 and 2 can be compared with the forward-facing radiated emission values measured from these same lights. The emission levels have to be measured at the frequencies the radios are tuned to during testing. AIS operates on both 161.975 and 162.025 MHz. The VHF radio was tested on channel 15 or 156.750 MHz, 50 kHz from the distress channel 16. Table 3 shows the radiated emission levels at 156.750 and 162 MHz. Note that radiated emission levels, VHF 4’ tests, VHF 8’ tests, and AIS tests were each performed and measured at different times, so variations in results will occur as interfering emissions shift and drift in frequency and intensity.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Light Sample Number | 20 kHz Average, dB µV/m at 1m | | | 120 kHz Average, dB µV/m at 1m | | | Polarization |
| Highest value | Value at 156.75 MHz | Value at 162 MHz | Highest value | Value at 156.75 MHz | Value at 162 MHz |
| 1 | 7 | 0 | 0 | 13 | 8 | 8 | Vertical |
| 2 | 21 | 12 | 10 | 23 | 13 | 12 | Horizontal |
| 3 | 25 | 16 | 18 | 24 | 22 | 10 | Vertical |
| 4 | 25 | 24 | 14 | 27 | 23 | 10 | Horizontal |
| 5 | 41 | 32 | 38 | 43 | 41 | 41 | Horizontal |
| 6 | 22 | 18 | 19 | 27 | 23 | 23 | Horizontal |
| 7 | 32 | 12 | 12 | 32 | 15 | 12 | Vertical |
| 8 | 9 | 4 | 7 | 14 | 11 | 10 | Horizontal |
| 10 | 25 | 20 | 13 | 29 | 21 | 18 | Vertical |

Table 3 - Radiated emission results

Test results are shown in Tables 4 (VHF receiver sensitivity) and 5 (AIS sensitivity), and plotted in Figures 1 and 2 respectively. Note the anomaly shown in the 20 kHz and 120 kHz RBW values shown for light sample #3 in Table 5, in which the 20 kHz RBW emission is 8 dB higher than the 120 kHz emission. That anomaly is better seen in the noise blip at 162 MHz in Figure 3, the original 20 kHz RBW emission plot. The 10 dB µV/m value shown at 162 MHz in Figure 4 is likely the actual value for both bandwidths. This anomaly illustrates the limits in making precise measurements in tests such as these.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Light Sample Number | Measured field strength at 1m at VHF channel 15  In dB µV/m | | Receiver sensitivity degradation, in dB | | | |
| 4’ (1.5m) whip | | 8’ (2.5m) whip | |
| At 1m | At 0.33m | At 1m | At 0.33m |
| 20 kHz RBW | 120 kHz RBW |
| 1 | 0 | 8 | 0 | 1 | 0 | 0 |
| 2 | 12 | 13 | 4 | 8 | 2 | 3 |
| 3 | 16 | 22 | 10 | 12 | 5 | 6 |
| 4 | 24 | 23 | 3 | 11 | 3 | 2 |
| 5 | 32 | 41 | 43.5 | 48.5 | 39.5 | 30.5 |
| 6 | 18 | 23 | 7 | 6 | 1 | 2 |
| 7 | 12 | 15 | 8.5 | 10.5 | 7.5 | 8.5 |
| 8 | 4 | 11 | 3 | 4 | 1 | 4 |
| 10 | 20 | 21 | 4 | 19 | 10 | 14 |

Table 4 – Radiated emission effect on VHF receiver sensitivity

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Light Sample Number | Measured field strength at 1m at 162 MHz  In dB µV/m | | Receiver sensitivity degradation, in dB | |
| At 1m | At 0.33m |
| 20 kHz RBW | 120 kHz RBW |
| 1 | 0 | 8 | 2 | 3 |
| 2 | 10 | 12 | 5 | 5 |
| 3 | 18 | 10 | 2 | 4 |
| 4 | 14 | 10 | 3 | 3 |
| 5 | 38 | 41 | 23 | 21 |
| 6 | 19 | 23 | 1 | 5 |
| 7 | 12 | 12 | 3 | 4 |
| 8 | 7 | 10 | 2 | 2 |
| 10 | 13 | 18 | 5 | 10 |

Table 5 – Radiated emission effect on AIS receiver sensitivity




Figure 1: VHF SINAD test results using a 4’ (1.5m) whip at 1m






Figure 2 – AIS test results using a 4’ (1.5m) whip at 1m



162 MHz

Figure 3 – Light sample #3, 20 kHz RBW AV, Vertical



162 MHz

Figure 4 – Light sample #3, 120 kHz RBW AV, Vertical

**Conclusion from test results:**

Although it is difficult to come to a precise conclusion, these tests appear to confirm the predicted radiated emission limit of 2 dB µV/m average at 20 kHz RBW, necessary to protect a VHF radio and AIS, as calculated in Section 2.1.3.2. It also shows that based upon the lights tested, a radiated emission limit of about 10 dB µV/m average at 120 kHz RBW should provide equivalent protection.

However, a review of emission limit necessary to protect the VHF Data Exchange System (VDES) satellite downlink as described in ANNEX 1 should also be considered.

**ANNEX 3**

**Review of Emission Limits in the GNSS Bands**

IEC 60945 Annex C states *“﻿Above 1 GHz the ship may be carrying receivers in the bands 1525 MHz – 1544 MHz for Inmarsat, 1575,42 MHz ± 1,023 MHz for GPS and 1602 MHz – 1615 MHz for GLONASS. The band 1525 MHz – 1544 MHz is used for GMDSS distress and safety. Similarly, Global Navigation Satellite Systems (GNSS) is becoming an IMO carriage requirement and the bands around 1575,42 MHz and 1602 MHz – 1615 MHz require protection. In this edition limits are therefore given in 9.3 extending to 2 GHz.”* IEC 60945 existing radiated emission limits were simply extended in its last edition from 1 GHz to 2 GHz to include GMDSS ship earth stations and GNSS shipboard receivers. New emission limits based upon Recommendations ITU-R M.1903-1, M.1905-1, M.1902-1 and RTCA DO-160G are considered.

**Current relevant EMC Standards**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Standard** | **Frequency  Band** | **Band-width** | **Distance** | **Emission limit** | | |
| **Quasi Peak[[18]](#footnote-18)** | **Average** | **Peak** |
| IEC 60945 | 1 to 2 GHz | 120 kHz | 3m | 54 dBµV/m | - | - |
| FCC Part 15 Class B | - | 1 MHz | 3m | - | 54 dBµV/m | 74 dBµV/m |
| CISPR 15[[19]](#footnote-19) | 1 to 6 GHz | 1 MHz | 3m | - | 50 dBµV/m | 70 dB µV/m |
| CISPR 25 Class 5 | BDS 1553-1569 MHz | 9 kHz | 1m | - | 5.5 dBµV/m | - |
| GPS 1567-1583 MHz | 9 kHz | 1m | - | 10 dBµV/m | - |
| GLONASS 1590-1617 MHz | 9 kHz | 1m | - | 10 dBµV/m | - |
| GPS L5 1156.45-1196.45 MHz | 9 kHz | 1m | - | 20 dB µV/m | - |
| MIL-STD-461G | ~1.5 GHz | 1 MHz | 1m | - | - | 60 dBµV/m |
| RTCA DO-160G | 1559-1610 MHz | 1 MHz | 1m | - | - | 40 dBµV/m |

**Recommendation ITU-R M.1903-1 at upper L-band**

Radiated emissions limits (EMI requirements) to protect GNSS (e.g., GPS) receivers should be based on Recommendation ITU-R M.1903-1 *Characteristics and protection criteria for receiving earth stations in the* *radionavigation-satellite service (space-to-Earth) and receivers in the aeronautical radionavigation service operating in the band 1 559-1 610 MHz*

Parameters used in this review was based upon ﻿Table 2 *Technical characteristics and protection criteria for RNSS receivers (space-to-Earth) operating in the 1 559-1 610 MHz band*, General purpose No. 1, aggregate wideband interference power density. ﻿Wideband continuous interference is considered to have a bandwidth greater than 1 MHz.


|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **GNSS Receiver Parameter** | **GPS** | **Galileo** | **GLONASS** | **BDS (Beidou)** |
| M1903 Table 2 receiver type | General purpose No. 1 | General purpose No. 1 | General purpose No. 1 | General purpose No. 2 |
| Frequency | ﻿1 575.42 ±  12 MHz | ﻿1 575.42 ± 12 MHz | ﻿ 1602 + 0.5625K  ± 5.11, where  K = −7, …, +6 | ﻿1 561.098  ± 2.046  1 589.742  ± 2.046 |
| Acquisition mode threshold power density level of aggregate wideband interference at the passive antenna output | -142 dBW/MHz =  -112 dBm/MHz | -142 dBW/MHz =  -112 dBm/MHz | -142 dBW/MHz =  -112 dBm/MHz | -146 dBW/MHz =  -116 dBm/MHz |
| ﻿Acquisition mode threshold power level of aggregate narrow-band  interference at the passive antenna output | -158 dBW = ‑128 dBm | -158 dBW = ‑128 dBm | -158 dBW = ‑128 dBm | -156 dBW = ‑126 dBm |
| Antenna gain | 6 dBi | 6 dBi | 6 dBi | 3 dBi |
| RF filter 3 dB bandwidth | 32 MHz | 32 MHz | 32 MHz | 4.196 MHz |
| Pre-correlation filter 3 dB bandwidth | 2 MHz | 2 MHz | 22 MHz | 4.096 MHz |

**GPS, GLONASS, Galileo and BDS L1 navigational frequency bands**

**ITU-R M.1903**

**ITU-R M.1902**

**ITU-R M.1905**



**Calculation of GNSS protection limits based upon Rec. ITU-R M.1903-1   
at upper L-band**

Antenna factor at 50 ohms

AF50Ω = 20 log10 fMHz – 10 log10 Gnumeric – 29.7707 dB/m, Gnumeric = 1.0 for 0 dBi[[20]](#footnote-20)

            = 63.945 –  29.7707 = 34.174 dB/m at 1575 MHz (GPS and Galileo)

= 64.093 –  29.7707 = 34.322 dB/m at 1602 MHz (GLONASS)

= 63.868 –  29.7707 = 34.097 dB/m at 1561 MHz (BDS)

P dBm      = V dB uV – 107 (power at the receiver input)

E dB µV/m = AF50Ω + V dB µV= AF50Ω + P dBm + 107 (field strength 1m from the antenna)

E dB µV/m = P dBm + 107 + 34.175 = P dBm + 141.175 (GPS and Galileo)

E dB µV/m = P dBm + 107 + 34.322 = P dBm + 141.323 (GLONAS)

E dB µV/m = P dBm + 107 + 34.097 = P dBm + 141.097 (BDS)

**GNSS protection criteria at 1m based upon Rec. ITU-R M.1903-1 wideband interference**

P dBm (WBacquisition) = -112 dBm/MHz + 10 log (2) = -109 dBm (GPS and Galileo)

P dBm (1MHz RBW) = -112 dBm/MHz - 10 log (1/1) = -112 dBm (GPS and Galileo)

P dBm (9 kHz RBW) = -112 dBm/MHz - 10 log (1/.009)[[21]](#footnote-21) = -132.46 dBm (GPS and Galileo)  
P dBm (WBacquisition) = -112 dBm/MHz + 10 log (22) = -98.6 dBm (GLONASS)

P dBm (1MHz RBW) = -112 dBm/MHz - 10 log (1/1) = -112 dBm (GLONASS)

P dBm (9 kHz RBW) = -112 dBm/MHz - 10 log (1/.009) = -132.46 dBm (GLONASS)

P dBm (WBacquisition) = -116 dBm/MHz + 10 log (4.096) = -109.9 dBm (BDS)

P dBm (1MHz RBW) = -116 dBm/MHz - 10 log (1/1) = -116 dBm (GLONASS)

P dBm (9 kHz RBW) = -116 dBm/MHz - 10 log (1/.009) = -136.46 dBm (GLONASS)

**GPS and Galileo**

**E dB µV/m (1 MHz) = -112 dBm + 141.175 = 29.2 dB µV/m**

**E dB µV/m (9 kHz) = -132.46 dBm + 141.175 = 8.7 dB µV/m**

**GLONASS**

**E dB µV/m (1 MHz) = -112 dBm + 141.323 = 29.3 dB µV/m**

**E dB µV/m (9 kHz) = -132.46 dBm + 141.323 = 8.9 dB µV/m**

**BDS**

**E dB µV/m (1 MHz) = -116 dBm + 141.097 = 25.1 dB µV/m (BDS)**

**E dB µV/m (9 kHz) = -136.46 dBm + 141.097 = 4.6 dB µV/m (BDS)**

**EMC protection criteria based upon Rec. ITU-R M.1903 narrowband interference**

E dB µV/m = AF50Ω + V dB µV= AF50Ω + P dBm + 107 (field strength 1m from the antenna)  
E dB µV/m = P dBm + 107 + 34.175 = P dBm + 141.175 (GPS and Galileo)

E dB µV/m = P dBm + 107 + 34.322 = P dBm + 141.323 (GLONAS)

E dB µV/m = P dBm + 107 + 34.097 = P dBm + 141.097 (BDS)

P dBm (NBacquisition) = -128 dBm (GPS and Galileo)  
P dBm (NBacquisition) = -128 dBm (GLONASS)

P dBm (NBacquisition) = -126 dBm (BDS)

**E dB µV/m (NBacquisition)**= -128 dBm + 141.175 = **13.2 dB µV/m** (GPS and Galileo)

**E dB µV/m (NBacquisition)**= -128 dBm + 141.323 = **13.3 dB µV/m** (GLONASS)

**E dB µV/m (NBacquisition)**= -126 dBm + 141.097 = **15.1 dB µV/m** (BDS)

**Comparison of ITU-R M.1903-1 based calculated emission limits   
with existing standards, normalized to 1m[[22]](#footnote-22)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EMC Standard** | **Resolution Bandwidth** | **EMC standard emission limit** | **M.1903 wideband** | | **M.1903 narrowband** | | **GNSS Receiver Distortion Distance[[23]](#footnote-23)** |
| **Emission requirement** | **Difference** | **Emission requirement** | **Difference** |
| IEC 60945 | 120 kHz | 63.5 dB µV/m QP | 20 dBµV/m  15.9 dBµV/m (BDS) | +43.5 dB  +44.5 dB (BDS) | 13.2 dB µV/m  15.1 dB µV/m (BDS) | +50.3 dB  +48.4 dB (BDS) | 100m+ |
| FCC Part 15 Class B | 1 MHz | 63.5 dB µV/m AV | 29.2 dBµV/m  25.1 dBµV/m (BDS) | +34.3 dB  +38.4 dB (BDS) | 13.2 dB µV/m  15.1 dB µV/m (BDS) | +50.3 dB  +48.4 dB (BDS) | 50m  (100m+ NB) |
| CISPR 15 (not yet adopted) | 1 MHz | 59.5 dB µV/m AV | 29.2 dBµV/m  25.1 dBµV/m (BDS) | +30.3 dB  +34.4 dB (BDS) | 13.2 dB µV/m  15.1 dB µV/m (BDS) | +46.3 dB  +44.4 dB (BDS) | 30m  (100m+ NB) |
| CISPR 25 Class 5 GNSS | 9 kHz | 10 dB µV/m AV  5.5 dB µV/m (BDS) | 8.7 dBµV/m  4.6 dBµV/m (BDS) | +1.3 dB  -0.9 dB (BDS) | 13.2 dB µV/m  15.1 dB µV/m (BDS) | -3.2 dB  -9.6 dB (BDS) | 1m |
| MIL-STD-461G | 1 MHz | 60 dBµV/m PK | 29.2 dBµV/m  25.1 dBµV/m (BDS) | +30.8 dB  +34.9 dB (BDS) | 13.2 dB µV/m  15.1 dB µV/m (BDS) | +46.8 dB  +44.9 dB (BDS) | 30m  (100m NB) |
| RTCA DO-160G | 1 MHz | 40 dBµV/m  PK | 29.2 dBµV/m  25.1 dBµV/m (BDS) | + 10.8 dB  + 14.9 dB (BDS) | 13.2 dB µV/m  15.1 dB µV/m (BDS) | +26.8 dB  +24.9 dB (BDS) | 3m  (20m NB) |

**Recommendations ITU-R M.1902-1 and M.1905-1 at lower L-band**

﻿Recommendation ITU-R M.1902-1 *Characteristics and protection criteria for receiving earth stations in the radionavigation-satellite service (space-to-Earth) operating in the band 1215 - 1300 MHz* addresses lower L-band GNSS system signals including GPS L2 and GLONASS G2. Recommendation ITU-R M.1905-1 *Characteristics and protection criteria for receiving earth stations in the radionavigation-satellite service (space-to-Earth) operating in the band 1164 - 1215 MHz* addresses lower L-band GNSS system signals including GPS L5 and Galileo E5.

R**ecommendation ITU-R M.1902-1**

|  |  |  |
| --- | --- | --- |
| **GNSS Receiver Parameter** | **GPS L2** | **GLONASS G2** |
| M1902 Table 1 receiver type | General purpose | General purpose |
| Frequency | ﻿﻿1 227.6 ± 12 MHz | ﻿ 1246 + 0.4375K  ± 5.11, where  K = −7, …, +6 |
| Acquisition mode threshold power density level of aggregate wideband interference at the passive antenna output | -145 dBW/MHz =  -115 dBm/MHz | -145 dBW/MHz =  -115 dBm/MHz |
| Acquisition mode threshold power level of aggregate narrow-band interference at the passive antenna output | -164 dBW =  ‑134 dBm | -164 dBW =  ‑134 dBm |
| Antenna gain | 6 dBi | 6 dBi |
| RF filter 3 dB bandwidth | 32 MHz | 30 MHz |
| Pre-correlation filter 3 dB bandwidth | 2 MHz | 20 MHz |

**Recommendation ITU-R M.1905-1**

|  |  |
| --- | --- |
| **GNSS Receiver Parameter** | **GPS L5 and Galileo E5** |
| M1905 Table 1 receiver type | General purpose |
| Frequency | ﻿﻿ ﻿1 207.14 ± 12  1 176.45 ± 12 MHz |
| Acquisition mode threshold power density level of aggregate wideband interference at the passive antenna output | -146 dBW/MHz =  -116 dBm/MHz |
| Acquisition mode threshold power level of aggregate narrow-band interference at the passive antenna output | -156 dBW =  ‑126 dBm |
| Antenna gain | 3 dBi |
| RF filter 3 dB bandwidth | 24 MHz |
| Pre-correlation filter 3 dB bandwidth | 20.46 MHz |

The parameters described in Rec. M.1902-1 and M.1905-1 are similar and comparable to those in Table 2 of Rec. M.1903-1.

AF50Ω = 20 log10 fMHz – 29.7707 dB/m = 32.01 dB/m (GPS L2)

= 32.14 dB/m (GLONASS G2)

= 31.86 dB/m (GPS L5 1207 MHz)

= 31.64 dB/m (GPS L5 1176 MHz)

32 dB/m

|  |  |  |  |
| --- | --- | --- | --- |
| **ITU-R Recommendation** | **Wideband interference** | **Narrowband interference** | **Antenna Factor** |
| M.1903 | -112 dBm/MHz | -128 dBm | 34 dB/m |
| M.1902 GPS L2/GLONASS G2 | -115 dBm/MHz | -134 dBm | 32 dB/m |
| M.1905 | -116 dBm/MHz | -126 dBm | 32 dB/m |

E dB µV/m = AF50Ω + P dBm + 107

**EMC protection criteria for GPS L2 and GLONASS G2 (M.1902)**

**E dB µV/m (1 MHz)(WB)**= **24 dB µV/m**

**E dB µV/m (9 kHz)(WB)**=  **4 dB µV/m**  
**E dB µV/m (NB) = 5 dB µV/m**

**EMC protection criteria for GPS L5 and Galileo E5 (M.1905)**

**E dB µV/m (1 MHz)**= **23 dB µV/m**

**E dB µV/m (9 kHz)**=  **3 dB µV/m**

**E dB µV/m (NB) = 13 dB µV/m**

**Ambient.** The EMI test laboratory ambient level at 9 kHz RBW using an average detector was about -2 to -1 dB µV/m.

**Conclusions**

Only CISPR 25 Class 5 and RTCA DO-160G appear designed to protect GNSS receivers from unintentional electromagnetic interference close to GNSS antennas.

**Radiated emission average (AV) limits:** Proposed that maritime applications adopt radiated emission limits based upon Recommendations ITU-R M.1903-1, M.1902-1 and M.1905-1 based upon receiver acquisition mode, aligned with those of CISPR 25 Class 5, in the relevant bands used by shipboard GNSS receivers.

**Radiated emission peak (PK) limits:** Proposed that maritime applications consider peak radiated emission limits based upon RTCA DO-160G.

**Radiated emission bandwidth:** Proposed that maritime applicationsadopt 9 kHz resolution bandwidth to ensure ITU-R M.1902, M.1903 and M.1905 narrowband emission limits are met, and aligned with CISPR 25.

**L-band GNSS emission limits with source**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Frequency band (MHz)** | **ITU-R Rec.** | **CISPR 25 Class 5 limits** | **ITU-R WB limits (9 kHz)** | **ITU-R NB Limits** | **RTCA DO-160G PK limits (1 MHz)** | **Maritime applications proposed AV limits** |
| 1559 - 1591 | M.1903 | 10 dB µV/m | 9 dB µV/m | 13 dB µV/m | 40 dB µV/m | 10 dB µV/m |
| 1593 - 1610 | M.1903 BDS | 5.5 dB µV/m | 5 dB µV/m | 15 dB µV/m | 40 dB µV/m | 5.5 dB µV/m |
| 1260 - 1300 | M.1902 | - | 4 dB µV/m | 5 dB µV/m | - | 10 dB µV/m |
| 1164 - 1214 | M.1905 | 20 dB µV/m | 3 dB µV/m | 13 dB µV/m | 38 dB µV/m | 20 dB µV/m |

1. These reports were received in response to USCG Marine Safety Alert, Bulletin 13-18 (see <https://www.dco.uscg.mil/Portals/9/DCO%20Documents/5p/CG-5PC/INV/Alerts/1318.pdf?ver=2018-08-16-091109-630>). [↑](#footnote-ref-1)
2. “Reference Data for Radio Engineers,” Fifth Edition, March 1970, Section 21-11 to 21-12. [↑](#footnote-ref-2)
3. H. Jin, W. Yang, F. Yu and Z. Wang, "A novel EBG structure with spiral line bridges for radiation suppression in marine VHF band," in IEEE Electromagnetic Compatibility Magazine, vol. 8, no. 4, pp. 56-61, 4th Quarter 2019. [↑](#footnote-ref-3)
4. Based on equations for average sidelobe levels for omnidirectional antennas in Recommendation [ITU-R F.1336-5](https://www.itu.int/rec/R-REC-F.1336/en), *recommends* 2.2. These patterns are for use in the far field, beyond the reactive near field. [↑](#footnote-ref-4)
5. RR Appendix 18 [↑](#footnote-ref-5)
6. Sponsored by the United States Coast Guard at IMANNA Laboratory, Inc. [www.imanna.com](http://www.omanna.com) [↑](#footnote-ref-6)
7. “Active” means that a switch-mode power supply is used to drive the LED light. [↑](#footnote-ref-7)
8. A more comprehensive review of emissions limits in the GNSS bands is provided in ANNEX 3. [↑](#footnote-ref-8)
9. Note that quasi-peak above 1 GHz is undefined and not recognized by CISPR. [↑](#footnote-ref-9)
10. Com-Power Corporation, Model PAM-6000, [ASSEMBLY PROCEDURE (com-power.com)](https://www.com-power.com/uploads/pdf/PAM-6000-2.pdf) [↑](#footnote-ref-10)
11. Amplifier Research Corporation, Model ATH800M6G, [Manual Text Template (arworld.us)](https://www.arworld.us/post/opMan/ATH800M6G.pdf) [↑](#footnote-ref-11)
12. These tests are included in the US Federal Communications Commission Ship Inspection Checklists available at <https://www.fcc.gov/eb-ship-inspection-checklists> and are also planned for inclusion in the next edition of NMEA 0400 Installation Standard. [↑](#footnote-ref-12)
13. Protection criteria for the VDES terrestrial components, including the AIS, are derived in Section 2.1.3. This analysis pertains to the VDES satellite components, which are the most vulnerable. [↑](#footnote-ref-13)
14. Test levels for the 9 kHz and the 120 kHz resolution bandwidths, are calculated from the 20 kHz level, assuming a Gaussian power flux density for the interference, which typically is not the case since the highest levels of interference on ships are typically from switch-mode power supplies with various non-Gaussian waveforms. Thus the 20 kHz resolution bandwidth is best suited for AIS protection criteria. [↑](#footnote-ref-14)
15. ibid [↑](#footnote-ref-15)
16. The VDES satellite downlink is a spread spectrum waveform. Thus the 120 kHz resolution bandwidth is best suited for VDES satellite downlink protection criteria. [↑](#footnote-ref-16)
17. This annex provides test results from the EMI test laboratory (refer to footnote 6) that apply to shipborne installations of the AIS and VHF GMDSS marine radios. [↑](#footnote-ref-17)
18. CISPR 16-1-1 does not recognize quasi-peak measurements above 1 GHz. [↑](#footnote-ref-18)
19. CISPR 15 Ed.9 currently has no emissions limits above 1 GHz. However, ﻿CIS/F/801/CD Amd.1 would raise emission limits to 6 GHz. Emission limits from 3 to 6 GHz would be 54 dB µV/m AV and 74 dB µV/m PK. [↑](#footnote-ref-19)
20. Assume 0 dBi since in worst case, gain equally affects both signal and interference. [↑](#footnote-ref-20)
21. 10 log is appropriate in this case, since ITU-R specified protection requirements as power flux density (dBW/MHz). [↑](#footnote-ref-21)
22. Peak, quasi-peak and average measurements are considered equivalent for this purpose. [↑](#footnote-ref-22)
23. The receiver distortion distance is the minimum separation distance between the victim receiver’s antenna and the unit capable of causing interference that is required in order to ensure that harmful interference is not caused to the receiver, assuming free space propagation loss. [↑](#footnote-ref-23)