|  |
| --- |
| U.S. Radiocommunications SectorFact Sheet |
| **Working Party:** ITU-R WP 5B | **Document No:** USWP5B27-21-FS |
| **Ref:** 5B/355-E Annex 25 | **Date:** August 12, 2021 |
| **Document Title:** Working Document towards a Preliminary Draft New [Report/Recommendation] ITU-R M.[AMRS-VDL], “Characteristics and protection criteria for the International Civil Aviation Organization standardized VHF datalink Mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136-137 MHz” |
| **Author(s)/Contributors(s):**Chris TourignyFAA Spectrum Engineering ServicesMichael TranMITRE | Phone: 202-267-3071Email: chris.tourigny@faa.govPhone: 703-983-1295 Email : mtran@mitre.org |
| **Purpose/Objective:** The purpose of this contribution is to provide updates to Document 5B/355 Annex 25 to mature the technical characteristics and protection criteria for the VHF datalink (VDL) systems operating in the frequency band 136 – 137 MHz, allocated to the aeronautical mobile (route) service. VDLM2 is internationally standardized by ICAO. |
| **Abstract:** This contribution provides updates to document 5B/355 Annex 25 on the technical characteristics and protection criteria for the VHF datalink Mode 2 (VDLM2) systems operating in the 136 – 137 MHz frequency band, allocated to the AM(R)S. |

|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Source: 5B/355-E Annex 25Subject: AM(R)S VDLM2 in 136 – 137 MHz | **Document 5B/** |
| **29 November 2021** |
| **English only** |
| United States of America |
| working document towards a preliminary draft neW [report/recommendation] itu-r m.[amRS-VDL]**Characteristics and protection criteria for the International Civil Aviation Organization standardized VHF datalink Mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136 – 137 MHz** |
|  |

**Introduction**

This contribution provides updates to Document 5B/355 Annex 25, on the technical characteristics and protection criteria for ICAO standardized VHF datalink (VDL) Mode 2 (VDLM2) operating in the aeronautical mobile (route) service in the frequency band 136 - 137 MHz.

Attachment: 1

ATTACHMENT

Working document towards a preliminary draft new [report/recommendation] ITU-r m.[amrs-vDL]

**Characteristics and protection criteria for the International Civil Aviation Organization standardized VHF datalink Mode 2 systems operating in the aeronautical mobile (route) service in the frequency band 136-137 MHz**