|  |
| --- |
| U.S. Radiocommunications SectorFact Sheet |
| **Working Party:** ITU-R WP5B | **Document No:** USWP5B25-FS-12 |
| **Ref:** Rec. ITU-R M.489-2  | **Date:** 11 September 2020 |
| Document Title: Proposed corrigendum to Recommendation ITU-R M.489-2 |
| **Author(s)/Contributors(s):**Joe HerseyJOECEL EngineeringRoss NorsworthyREC IncJerry UlcekUS Coast Guard | **Email**: joe@joecel.com**Phone**: (301) 512-9860**Email**: ross\_norsworthy@msn.com**Phone**: (757) 515-8025**Email**: jerry.l.ulcek@uscg.mil**Phone**: (202) 475-3551 |
| **Purpose/Objective:** Clarify and correct what has become by some a misunderstanding in the difference between signal and noise plus distortion ratio (SINAD) and signal-to-noise ratio in the measurement of receiver performance. |
| **Abstract:** Rec. ITU-R M.489-2 ﻿*Technical characteristics of VHF radiotelephone**equipment operating in the maritime mobile service in channels spaced by 25 kHz* requirement for receiver sensitivity “for a given reference signal-to-noise ratio at the output of the receiver” has long been properly understood to mean a SINAD measurement, and is rightly interpreted that way by applicable test standards. Yet over time some have misinterpreted that understanding and a clarification may now be warranted. The clarification might be simply accomplished editorially or by corrigendum. |