|  |  |
| --- | --- |
| U.S. Radiocommunications Sector  Fact Sheet | |
| **Working Party:** ITU-R WP 4C | **Document No:** USWP4C-11 |
| **Ref:** N/A | **Date:** 22 Mar 2024 |
| Document Title: Working Document [AI 1.13 sharing and compatibility studies] | |
| **Author(s)/Contributors(s):**  Jameson Dempsey  SpaceX  Zahid Islam  SpaceX  Brett Tarnutzer  SpaceX  Pascale Dumit  T-Mobile | Email: [Jameson.Dempsey@spacex.com](mailto:Jameson.Dempsey@spacex.com)  Phone:  Email: [km.islam@spacex.com](mailto:km.islam@spacex.com)  Phone:  Email: [brett.tarnutzer@spacex.com](mailto:brett.tarnutzer@spacex.com)  Phone:  Email: [Pascale.Dumit@T-Mobile.com](mailto:Pascale.Dumit@T-Mobile.com)  Phone: |
| **Purpose/Objective:** Initiate the work under WRC-27 Agenda Item 1.13 | |
| **Abstract:** The proposed U.S. contribution aims at getting the work started under WRC-27 Agenda Item 1.13.  The document also includes a skeleton of various sections for the Working Document for the sharing and compatibility studies to be conducted under WRC-27 Agenda Item 1.13. | |

|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Source: -  Subject: WRC-27 agenda item 1.13 | **Document 4C/TBD** |
| **TBD May 2024** |
| **English only** |
| United States of America | |
| WORKING DOCUMENT [AI 1.13 SHARING AND COMPATIBILITY STUDIES] | |
|  | |

Introduction

The proposed U.S. contribution aims at getting the work started under WRC-27 Agenda Item 1.13. The attached document includes a skeleton of the envisaged sections for conducting the sharing and compatibility studies under WRC-23 Agenda Item 1.13 in bands between 694 - 2 700 MHz identified for IMT in the Radio Regulations and reflected in Recommendation ITU-R M.1036.

**Attachment:** 1

|  |
| --- |
| Attachment 1 |
| WORKING DOCUMENT [AI 1.13 SHARING AND COMPATIBILITY STUDIES] |

1. **Introduction**

Resolution 253 (WRC-23) calls for studies on possible new allocations to the mobile-satellite service for direct connectivity between space stations and International Mobile Telecommunications (IMT) user equipment to complement terrestrial IMT network coverage.

Studies on sharing and compatibility between incumbent services, including in adjacent frequency bands are essential to ensure the protection of incumbent services in accordance with the Radio Regulations.

1. **Information on IMT frequency arrangements contained in**

**Recommendation ITU-R M.1036 and the corresponding incumbent and adjacent band services**

The following tables provide information on the IMT frequency arrangements contained in Recommendation ITU-R M.1036 with all the corresponding incumbent and adjacent band services for bands between 694 - 2 700 MHz identified for IMT in the Radio Regulations.

The tables for the Earth-to-space direction have been included for information. Depending on further analysis, studies for this direction might not be necessary given that the characteristics of the IMT mobile stations (i.e. user equipment) are envisaged to remain unchanged.

**[Editor's note:** The table for the Earth-to-space direction is included for information. Depending on further analysis, studies for this direction might not be necessary.**]**

|  |  |
| --- | --- |
| **FDD Frequency arrangements** | **Mobile station transmitter/  (Earth-to-space direction)  (MHz)** |
| A1 | 824-849 |
| A2 | 880-915 |
| A3 | 832-862 |
| A4 | 698-716 |
| 776-793 |
| A5 | 703-748 |
| A7 | 703-733 |
| A8 | 698-703 |
| A9 | 733-736 |
| A11 | 703-733 |

|  |  |  |  |
| --- | --- | --- | --- |
| **FDD Frequency arrangements** | **Base station transmitter/ (space-to-Earth direction) (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| A1 | 869-894 | FIXED  MOBILE  MOBILE except aeronautical  mobile  BROADCASTING  Radiolocation | FIXED  MOBILE  MOBILE except aeronautical  mobile  BROADCASTING  Radiolocation |
| A2 | 925-960 | FIXED  MOBILE  MOBILE except aeronautical  mobile  BROADCASTING  Radiolocation  Amateur | FIXED  MOBILE  MOBILE except aeronautical  mobile  BROADCASTING  Radiolocation  Amateur  AERONAUTICAL MOBILE (R)  AERONAUTICAL RADIONAVIGATION |
| A3 | 791-821 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| A4 | 728-746 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| 746-763 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| A5 | 758-803 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| A7 | 758-788 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| A8 | 753-758 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| A9 | 788-791 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| A10 | 738-758 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| A11 | 758-788 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |
| 738-758 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |

|  |  |  |  |
| --- | --- | --- | --- |
| **TDD Frequency arrangements** | **Un-paired arrangement (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| A6 | 698-806 | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING | FIXED  MOBILE except aeronautical  Mobile  MOBILE  BROADCASTING |

**[Editor's note:** The table for the Earth-to-space direction is included for information. Depending on further analysis, studies for this direction might not be necessary.**]**

|  |  |
| --- | --- |
| **FDD Frequency arrangements** | **Mobile station transmitter/  (Earth-to-space direction)  (MHz)** |
| G2 | 1 427-1 470 |

|  |  |  |  |
| --- | --- | --- | --- |
| **FDD Frequency arrangements** | **Base station transmitter/ (space-to-Earth direction) (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| G1 | 1 427-1 517 | SPACE OPERATION (Earth-to-space)  FIXED  MOBILE except aeronautical  MOBILE  BROADCASTING  BROADCASTING-SATELLITE | EARTH EXPLORATION-SATELLITE (passive)  RADIO ASTRONOMY  SPACE RESEARCH (passive)  FIXED  MOBILE except aeronautical  MOBILE  MOBILE-SATELLITE  (space-to-Earth) |
| G2 | 1 475-1 518 | FIXED  MOBILE except aeronautical  MOBILE  BROADCASTING  BROADCASTING-SATELLITE | BROADCASTING  BROADCASTING-SATELLITE  FIXED  MOBILE  MOBILE except aeronautical  mobile  MOBILE-SATELLITE  (space-to-Earth) |

|  |  |  |  |
| --- | --- | --- | --- |
| **TDD Frequency arrangements** | **Un-paired arrangement (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| G3 | 1 427-1 517 | SPACE OPERATION (Earth-to-space)  FIXED  MOBILE except aeronautical  MOBILE  BROADCASTING  BROADCASTING-SATELLITE | EARTH EXPLORATION-SATELLITE (passive)  RADIO ASTRONOMY  SPACE RESEARCH (passive)  FIXED  MOBILE except aeronautical  MOBILE  MOBILE-SATELLITE  (space-to-Earth) |

**[Editor's note:** The table for the Earth-to-space direction is included for information. Depending on further analysis, studies for this direction might not be necessary.**]**

|  |  |
| --- | --- |
| **FDD Frequency arrangements** | **Mobile station transmitter/  (Earth-to-space direction)  (MHz)** |
| B1 | 1 920-1 980 |
| B2 | 1 710-1 785 |
| B3 | 1 850-1 920 |
| B4 | 1 710-1 785 |
| 1 920-1 980 |
| B5 | 1 850-1 920 |
| 1 710-1 780 |
| B6 | 1 980-2 010 |
| B7 | 2 000-2 020 |

|  |  |  |  |
| --- | --- | --- | --- |
| **FDD Frequency arrangements** | **Base station transmitter/ (space-to-Earth direction) (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| B1 | 2 110-2 170 | FIXED  MOBILE  SPACE RESEARCH (deep space) (Earth-to-space)  MOBILE-SATELLITE  (space-to-Earth)  Mobile-Satellite (space-to-Earth) | SPACE OPERATION (Earth-to-space) (space-to-space)  EARTH EXPLORATION-SATELLITE (Earth-to-space) (space-to-space)  FIXED  MOBILE  SPACE RESEARCH (Earth-to-space) (space-to-space)  MOBILE-SATELLITE (space-to-Earth) |
| B2 | 1 805-1 880 | FIXED  MOBILE | FIXED  MOBILE |
| B3 | 1 930-2 000 | FIXED  MOBILE  MOBILE-SATELLITE (Earth-to-space)  Mobile-Satellite (Earth-to-Space) | FIXED  MOBILE  MOBILE-SATELLITE (Earth-to-space) |
| B4 | 1 805-1 880 | FIXED  MOBILE | FIXED  MOBILE |
| 2 110-2 170 | FIXED  MOBILE  SPACE RESEARCH (deep space) (Earth-to-space)  MOBILE-SATELLITE  (space-to-Earth)  Mobile-Satellite (space-to-Earth) | SPACE OPERATION (Earth-to-space) (space-to-space)  EARTH EXPLORATION-SATELLITE (Earth-to-space) (space-to-space)  FIXED  MOBILE  SPACE RESEARCH (Earth-to-space) (space-to-space)  MOBILE-SATELLITE (space-to  Earth) |
| B5 | 1 930-2 000 | FIXED  MOBILE  MOBILE-SATELLITE (Earth-to-space)  Mobile-Satellite (Earth-to-Space) | FIXED  MOBILE  MOBILE-SATELLITE (Earth-to-space) |
| 2 110-2 180 | FIXED  MOBILE  SPACE RESEARCH (deep space) (Earth-to-space)  MOBILE-SATELLITE  (space-to-Earth)  Mobile-Satellite (space-to-Earth) | SPACE OPERATION (Earth-to-space) (space-to-space)  EARTH EXPLORATION-SATELLITE (Earth-to-space) (space-to-space)  FIXED  MOBILE  SPACE RESEARCH (Earth-to-space) (space-to-space)  MOBILE-SATELLITE (space-to  Earth) |
| B6 | 2 170-2 200 | FIXED  MOBILE  MOBILE-SATELLITE (space-to-Earth) | SPACE OPERATION (space-to-Earth) (space-to-space)  EARTH EXPLORATION-SATELLITE (space-to-Earth) (space-to-space)  FIXED  MOBILE  SPACE RESEARCH (space-to-Earth) (space-to-space) |
| B7 | 2 180-2 200 | FIXED  MOBILE  MOBILE-SATELLITE (space-to-Earth) | SPACE OPERATION (space-to-Earth) (space-to-space)  EARTH EXPLORATION-SATELLITE (space-to-Earth) (space-to-space)  FIXED  MOBILE  SPACE RESEARCH (space-to-Earth) (space-to-space) |

|  |  |  |  |
| --- | --- | --- | --- |
| **TDD Frequency arrangements** | **Un-paired arrangement (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| B1 | 1 880-1 920 | FIXED  MOBILE | FIXED  MOBILE |
| 2 010-2 025 | FIXED  MOBILE  MOBILE-SATELLITE  (Earth-to-space) | MOBILE-SATELLITE (Earth-to-space)  SPACE OPERATION (Earth-to-space) (space-to-space)  EARTH EXPLORATION-SATELLITE (Earth-to-space) (space-to-space)  FIXED  MOBILE  SPACE RESEARCH (Earth-to-space) (space-to-space) |
| B3 | 1 920-1 930 | FIXED  MOBILE | FIXED  MOBILE |
| B4 | 1 880-1 920 | FIXED  MOBILE | FIXED  MOBILE |
| 2 010-2 025 | FIXED  MOBILE  MOBILE-SATELLITE  (Earth-to-space) | MOBILE-SATELLITE (Earth-to-space)  SPACE OPERATION (Earth-to-space) (space-to-space)  EARTH EXPLORATION-SATELLITE (Earth-to-space) (space-to-space)  FIXED  MOBILE  SPACE RESEARCH (Earth-to-space) (space-to-space) |
| B5 | 1 920-1 930 | FIXED  MOBILE | FIXED  MOBILE |

|  |  |  |  |
| --- | --- | --- | --- |
| **TDD Frequency arrangements** | **Un-paired arrangement (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| E1 | 2 300-2 400 | FIXED  MOBILE  RADIOLOCATION  Amateur | FIXED  MOBILE  MOBILE except aeronautical mobile  SPACE RESEARCH (deep space) (space-to-Earth)  RADIOLOCATION |

**[Editor's note:** The table for the Earth-to-space direction is included for information. Depending on further analysis, studies for this direction might not be necessary.**]**

|  |  |
| --- | --- |
| **FDD Frequency arrangements** | **Mobile station transmitter/  (Earth-to-space direction)  (MHz)** |
| C1 | 2 500-2 570 |
| C2 | 2 500-2 570 |

|  |  |  |  |
| --- | --- | --- | --- |
| **FDD Frequency arrangements** | **Base station transmitter/ (space-to-Earth direction) (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| C1 | 2 620-2 690 | FIXED  MOBILE except aeronautical  mobile  BROADCASTING-SATELLITE  FIXED-SATELLITE  (Earth-to-space)  (space-to-Earth)  Earth exploration-satellite  (passive)  Radio astronomy  Space research (passive) | FIXED  MOBILE except aeronautical  mobile  BROADCASTING-SATELLITE  FIXED-SATELLITE  (space-to-Earth)  EARTH EXPLORATION-SATELLITE (passive)  RADIO ASTRONOMY  SPACE RESEARCH (passive) |
| C2 | 2 620-2 690 | FIXED  MOBILE except aeronautical  mobile  BROADCASTING-SATELLITE  FIXED-SATELLITE  (Earth-to-space)  (space-to-Earth)  Earth exploration-satellite  (passive)  Radio astronomy  Space research (passive) | EARTH EXPLORATION-SATELLITE (passive)  RADIO ASTRONOMY  SPACE RESEARCH (passive) |
| 2 570-2 620 | FIXED  MOBILE except aeronautical  mobile  BROADCASTING-SATELLITE  FIXED-SATELLITE  (space-to-Earth) | FIXED  MOBILE except aeronautical  mobile  BROADCASTING-SATELLITE  FIXED-SATELLITE  (space-to-Earth) |

|  |  |  |  |
| --- | --- | --- | --- |
| **TDD Frequency arrangements** | **Un-paired arrangement (MHz)** | **Incumbent**  **Services** | **Adjacent band**  **Services** |
| C3 | 2500-2690 | FIXED  FIXED-SATELLITE (space-to-  Earth)  MOBILE except aeronautical  mobile  MOBILE-SATELLITE (space-to-Earth)  BROADCASTING-SATELLITE  FIXED-SATELLITE  (Earth-to-space)  (space-to-Earth)  Earth exploration-satellite  (passive)  Radio astronomy  Space research (passive) | FIXED  MOBILE  MOBILE-SATELLITE  (space-to-Earth)  RADIODETERMINATIONSATELLITE  (space-to-Earth)  RADIOLOCATION  EARTH EXPLORATION-SATELLITE (passive)  RADIO ASTRONOMY  SPACE RESEARCH (passive) |

1. **Detailed list of sharing studies to be conducted**

TBD

1. **Orbit and RF emission characteristics of systems and networks intended to provide direct connectivity between space stations and IMT user equipment**

The following tables summarize orbit configurations of systems and networks intended to provide direct connectivity between space stations and IMT user equipment.

Table X: TBD

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Altitude (km) | Inclination (deg) | # Planes | Sats per plane | RAAN spacing (deg) | Total number of sats |
|  |  |  |  |  |  |

TBD

**4.1 Emissions in the space-to-Earth direction**

This section will contain relevant emission characteristics of the space station to conduct sharing studies. Relevant parameters should include, among others:

* Power Flux Density on the ground
* Satellite antenna pattern
* Cell edge definition (relative to cell center)
* TBD

TBD

**4.2 Out-of-band emissions to be used for out-of-band studies**

This section contains relevant information on out-of-band emissions.

TBD

**4.3 Emissions in the Earth-to-space direction**

The intended operations foresee communications from unmodified user equipment. Consequently, the receive/transmit characteristics of the user equipment will remain unchanged with respect to standard terrestrial operations.

**4.4 Modelling of operations and the concept of topology**

This section will contain important assumptions on how to accurately model operations of systems and networks implementing direct-to-device communications.

**4.4.1 Satellite selection mechanism**

TBD

**4.4.2 The “topology” function**

Satellite operators use software-based systems to dynamically manage interference and remain within applicable limits to protect all relevant services.

Modelling topology is fundamental and should be duly taken into account in studies, as this is something satellite systems will implement continuously to manage interference into neighboring countries.

**4 Results of sharing studies**

TBD